# Other procedures (OTH)

## OTH.DEPTrain departure (DEP)

OTH.DEP.1At the initial station or after a scheduled stop the driver is allowed to depart when the following conditions are fulfilled:

1. after the driver has received an authorisation for train movement;
2. after train service conditions are fulfilled;
3. when it is time to depart, except when allowed to start before the scheduled time.

OTH.DEP.2If the driver has not received an authorisation for train movement at the expected time, and has no information as to the reason, the driver shall inform the signaller.

## OTH.TAFTrack Ahead Free (TAF)

OTH.TAF-[L2].1When the Track Ahead Free symbol (DR02) is displayed, the driver is allowed to confirm that the track ahead is free if the driver can ascertain that the track section between the head of the train and the next trackside signal, or ETCS stop marker/ETCS location marker is free.

DR02: Track Ahead Free

OTH.TAF-[L2.T].1To acknowledge the track ahead free request given by the RBC, the driver shall press the button associated with the symbol DR02 as indicated in the Figure OTH.TAF-[L2.T].F1.

Figure OTH.TAF-[L2.T].F1: Track Ahead Free Information (touch screen technology)

OTH.TAF-[L2.S].1To acknowledge the track ahead free request given by the RBC, the driver shall press the button associated with the symbol DR02 as indicated in the Figure OTH.TAF-[L2.S].F1.

Figure OTH.TAF-[L2.S].F1: Track Ahead Free Information (soft key technology)

OTH.TAF-[L2].2When the driver acknowledges the track ahead free request, the request is removed from the DMI display and the RBC is informed that the track ahead is free.

OTH.TAF-[L2].3If the driver does not acknowledge the track ahead free request, there is no restrictive consequence by the ETCS on-board system.

## OTH.DATChanging Train Data (DAT)

OTH.DAT.1The train data can be acquired from either driver input, pre-configured values or ERTMS/ETCS external sources.

### OTH.DAT.MANManual change of train data (MAN)

OTH.DAT.MAN.1After each modification of the composition of the train and after a technical problem that leads to a modification of the train data, the driver shall:

1. determine the new train data,
2. enter the new train data,
3. validate the new train data.

The driver shall never be involved in the modification/validation of the Train Data Traction system(s) accepted by the engine, List of National Systems available on-board or Axle number.

To enter, modify and revalidate the Train data, first the driver shall access the Main window.

During the Start of Mission procedure, the Main window is presented to the driver directly without the driver having to access it.

OTH.DAT.MAN-[T].1In case an operational data check rule is not satisfied at the end of the data entry as indicated in section CNT.DMI.GEN General description (GEN),, the “Yes” button attached to the question “Train data entry complete?” becomes a delay-type button, meaning that the driver must maintain it pressed for 2 seconds, to allow the driver to overrule the operational range check rule. The entered data values of the input fields concerned by the cross-check rule shall be considered as permitted and the data part of the corresponding echo texts displays the entered data values instead of ‘????’.

OTH.DAT.MAN-[S].1In case an operational data check rule is not satisfied at the end of the data entry as indicated in section CNT.DMI.GEN General description (GEN), the button attached to the question “Train data entry complete?” becomes a delay-type button, meaning that the driver must maintain it pressed for 2 seconds, to allow the driver to overrule the operational range check rule. The entered data values of the input fields concerned by the cross-check rule shall be considered as permitted and the data part of the corresponding echo texts displays the entered data values instead of ‘????’.

OTH.DAT.MAN-[L0N1.T].1To get access to the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L0N1.T].F2.

Figure MAIN-[L0N1.T].F2: Main button on Default window (touch screen technology)

OTH.DAT.MAN-[L2.T].1To get access to the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L2.T].F2.

Figure MAIN-[L2.T].F2: Main button on Default window (touch screen technology)

OTH.DAT.MAN-[L0N1.S].1To get access to the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L0N1.S].F2.

Figure MAIN-[L0N1.S].F2: Main button on Default window (soft key technology)

OTH.DAT.MAN-[L2.S].1To get access to the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L2.S].F2.

Figure MAIN-[L2.S].F2: Main button on Default window (soft key technology)

OTH.DAT.MAN-[B3241.L0N1.T].2The driver shall then select button on the Main window as indicated in Figure OTH.DAT.MAN-[B3241.L0N1.T].F2.

Figure OTH.DAT.MAN-[B3241.L0N1.T].F2: Train data button on Main window (touch screen technology)

OTH.DAT.MAN-[B3241.L2.T].2The driver shall then select button on the Main window as indicated in Figure OTH.DAT.MAN-[B3241.L2.T].F2.

Figure OTH.DAT.MAN-[B3241.L2.T].F2: Train data button on Main window (touch screen technology)

OTH.DAT.MAN-[B3241.L0N1.S].2The driver shall then select the button associated to the Train Data label on the Main window as indicated in Figure OTH.DAT.MAN-[B3241.L0N1.S].F2.

Figure OTH.DAT.MAN-[B3241.L0N1.S].F2: Train data button on Main window (soft key technology)

OTH.DAT.MAN-[B3241.L2.S].2The driver shall then select the button associated to the Train Data label on the Main window as indicated in Figure OTH.DAT.MAN-[B3241.L2.S].F2.

Figure OTH.DAT.MAN-[B3241.L2.S].F2: Train data button on Main window (soft key technology)

OTH.DAT.MAN-[B3M1.L0N1.T].1The driver shall then select button on the Main window as indicated in Figure OTH.DAT.MAN-[B3M1.L0N1.T].F1.

Figure OTH.DAT.MAN-[B3M1.L0N1.T].F1: Train data button on Main window (touch screen technology)

OTH.DAT.MAN-[B3M1.L23.T].1The driver shall then select button on the Main window as indicated in Figure OTH.DAT.MAN-[B3M1.L23.T].F1.

Figure OTH.DAT.MAN-[B3M1.L23.T].F1: Train data button on Main window (touch screen technology)

OTH.DAT.MAN-[B3M1.L0N1.S].1The driver shall then select the button associated to the Train Data label on the Main window as indicated in Figure OTH.DAT.MAN-[B3M1.L0N1.S].F1.

Figure OTH.DAT.MAN-[B3M1.L0N1.S].F1: Train data button on Main window (soft key technology)

OTH.DAT.MAN-[B3M1.L2.S].1The driver shall then select the button associated to the Train Data label on the Main window as indicated in Figure OTH.DAT.MAN-[B3M1.L2.S].F1.

Figure OTH.DAT.MAN-[B3M1.L2.S].F1: Train data button on Main window (soft key technology)

OTH.DAT.MAN-[112021].1As a result, the first Train data window is presented to the driver to initiate the entry of train data.

The Train data button is enabled to modify the train data when:

1. The train is at standstill AND
2. The Driver ID and ERTMS/ETCS level are valid AND
3. The mode is SB, FS, LS, SR, OS, UN, SN.

OTH.DAT.MAN-[22].1As a result, the first Train data window is presented to the driver to initiate the entry of train data.

The Train data button is enabled to modify the train data when:

1. The train is at standstill AND
2. The Driver ID and ERTMS/ETCS level are valid AND
3. The mode is SB, FS, LS, SR, OS, UN, SN, AD.

OTH.DAT.MAN-[30].1As a result, the first Train data window is presented to the driver to initiate the entry of train data.

The Train data button is enabled to modify the train data when:

1. The train is at standstill AND
2. The Driver ID and ERTMS/ETCS level are valid AND
3. The mode is SB, FS, LS, SR, OS, UN, SN, AD AND
4. Safe consist length information is not available OR [safe consist length information is available AND safe consist length values in front the engine are equal to zero].

OTH.DAT.MAN-[B41.V].1The number of modifiable elements of train data depend on the pre-configuration of the ETCS on-board equipment and the data received from external sources.

There are three types of train data entry configurations available to be used for the driver:

1. Fixed train data entry: the Train data window contains only one input field allowing the driver to enter a train type amongst a number of pre-configured ones. Each train type represents a combination of all train data. Once a train type is selected, the driver cannot change any value of a specific train data composing the selected train type.
2. Flexible train data entry: the Train data window(s) contain one or more input fields for the specific train data that the driver has to enter/modify.
3. Switchable train data entry: with this configuration, the driver can switch from a Fixed train data entry layout to a Flexible train data entry layout or vice versa.

For each train data it shall be configurable if the train data shall be provided from pre-configured values or from the driver according to “type of train data entry” information or via train interface with the train data themselves or via train interface derived from the “type of train configuration” information.

OTH.DAT.MAN-[B3.V].1The number of modifiable elements of train data depend on the pre-configuration of the ETCS on-board equipment and the data received from external sources.

There are three types of train data entry configurations available to be used for the driver:

1. Fixed train data entry: the Train data window contains only one input field allowing the driver to enter a train type amongst a number of pre-configured ones. Each train type represents a combination of all train data. Once a train type is selected, the driver cannot change any value of a specific train data composing the selected train type.
2. Flexible train data entry: the Train data window(s) contain one or more input fields for the specific train data that the driver has to enter/modify.
3. Switchable train data entry: with this configuration, the driver can switch from a Fixed train data entry layout to a Flexible train data entry layout or vice versa.

OTH.DAT.MAN-[T.V].1Figure OTH.DAT.MAN-[T.V].F1 shows an example of Train data window with Fixed Train data entry configuration.

Figure OTH.DAT.MAN-[T.V].F1: Fixed train data entry configuration (touch screen technology)

OTH.DAT.MAN-[S.V].1Figure OTH.DAT.MAN-[S.V].F1 shows an example of Train data window with Fixed Train data entry configuration.

Figure OTH.DAT.MAN-[S.V].F1: Fixed train data entry configuration (soft key technology)

OTH.DAT.MAN-[T.V].2Figure OTH.DAT.MAN-[T.V].F2 shows an example of Train data window with Flexible Train data entry configuration.

Figure OTH.DAT.MAN-[T.V].F2: Flexible train data entry configuration (touch screen technology)

OTH.DAT.MAN-[S.V].2Figure OTH.DAT.MAN-[S.V].F2 shows an example of Train data window with Flexible Train data entry configuration.

Figure OTH.DAT.MAN-[S.V].F2 : Flexible train data entry configuration (soft key technology)

OTH.DAT.MAN.2To enter, modify and revalidate each of the train data that requires driver validation, the driver shall follow the same sequence operations regardless of the type of train data entry configuration.

OTH.DAT.MAN-[T].2The driver shall select the input field to enter by pressing on it (if there is more than one) (1), then select the appropriate option within the available list or enter the train data value using the associated keyboard (2) if it is a numerical data and finally confirm the entry by pressing the button (3).

OTH.DAT.MAN-[T.V].3Figure OTH.DAT.MAN-[T.V].F3 shows an example of the operation sequence to enter or modify a train data.

Figure OTH.DAT.MAN-[T.V].F3: Steps to enter a train data (touch screen technology)

OTH.DAT.MAN-[S].2The driver shall select the input field to enter by using the and buttons (if there is more than one) (1), then select the appropriate option within the available list or enter the train data value using the associated keyboard (2) and finally confirm the selection by pressing the button (3).

OTH.DAT.MAN-[S.V].3Figure OTH.DAT.MAN-[S.V].F3 shows an example of the operation sequence to enter or modify a train data.

Figure OTH.DAT.MAN-[S.V].F3: Steps to enter a train data (soft key technology)

OTH.DAT.MAN.3To pass from one window to other, the driver shall press the and buttons.

OTH.DAT.MAN.4If there is only one possible data, it appears selected by default. When there are more than one, the first from this list is presented as selected by default.

OTH.DAT.MAN-[V].2With the Switchable train data configuration, the driver can change from Flexible train data entry configuration to Fixed train data entry configuration.

OTH.DAT.MAN.5The Train data window which is presented by default in the last used layout (i.e. the layout Fixed train data entry or Flexible train data entry).

OTH.DAT.MAN-[V].3To change the layout of the train data entry, the driver shall press the button or button. If the Train data windows show a Flexible train data entry layout (several input field available to be modified), the driver shall press the button. If the Train data windows show a Fixed train data entry layout (single entry field available to enter the train category), the driver shall press the button.

OTH.DAT.MAN-[T.V].4Figure OTH.DAT.MAN-[T.V].F4 shows an example of a Train data window with Switchable Train data entry configuration with the Select type button.

Figure OTH.DAT.MAN-[T.V].F4: Select type button on Switchable train data entry configuration (touch screen technology)

OTH.DAT.MAN-[S.V].4Figure OTH.DAT.MAN-[S.V].F4 shows an example of a Train data window with Switchable Train data entry configuration with the Select type button.

Figure OTH.DAT.MAN-[S.V].F4: Select type button on Switchable train data entry configuration (soft key technology)

OTH.DAT.MAN-[T.V].5Figure OTH.DAT.MAN-[T.V].F5 shows an example of Train data window with Switchable Train data entry configuration with the Enter data button.

Figure OTH.DAT.MAN-[T.V].F5: Enter data button on Switchable train data entry configuration (touch screen technology)

OTH.DAT.MAN-[S.V].5Figure OTH.DAT.MAN-[S.V].F5 shows an example of Train data window with Switchable Train data entry configuration with the Enter data button.

Figure OTH.DAT.MAN-[S.V].F5: Enter data button on Switchable train data entry configuration (soft key technology)

OTH.DAT.MAN.6Although, the driver presses the button to accept the train data, it is not validated yet and consequently the train data are not stored. The driver shall validate or not validate the data in a next step by using the Train data validation window which is presented to the driver.

OTH.DAT.MAN-[T.V].6To validate the Train data entered the driver shall press the button on the Validate train data window as indicated in Figure OTH.DAT.MAN-[T.V].F6. The Yes value is presented by default.

Figure OTH.DAT.MAN-[T.V].F6: Validate train data window (touch screen technology)

OTH.DAT.MAN-[S.V].6To validate the Train data entered the driver shall press the button on the Validate train data window as indicated in Figure OTH.DAT.MAN-[S.V].F6. The Yes value is presented by default.

Figure OTH.DAT.MAN-[S.V].F6: Validate train data window (soft key technology)

OTH.DAT.MAN.7If the No button is selected by the driver, the first Train data window is presented to the driver again with the previously entered train data proposed.

OTH.DAT.MAN-[112021.V].1Once the driver presses the Yes button to validate the train data entry, when the driver must enter at least one NTC data, the National data entry selection window is displayed.

The Hour Glass symbol (ST05) is displayed to indicate to the driver that the ETCS on-board equipment awaits answers from all the connected STMs supporting NTCs that need specific data.

OTH.DAT.MAN-[2230.V].1Once the driver presses the Yes button to validate the train data entry, when the driver must enter at least one NTC data, or ATO data, the Specific data entry selection window is displayed.

The Hour Glass symbol (ST05) is displayed to indicate to the driver that the ETCS on-board equipment awaits answers from all the connected STMs supporting NTCs that need specific data or from the ATO on-board that needs specific data.

OTH.DAT.MAN-[112021.L0N1.T.V].1When the Hour Glass symbol (ST05) disappears, the National data entry selection window offers the possibility to the driver to select , ... (1) and (2) as indicated in Figure OTH.DAT.MAN-[112021.L0N1.T.V].F1.

Figure OTH.DAT.MAN-[112021.L0N1.T.V].F1: National data entry selection window (touch screen technology)

OTH.DAT.MAN-[2230.L0N1.T.V].1When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select NTC A , NTC B (1) and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L0N1.T.V].F1.

Figure OTH.DAT.MAN-[2230.L0N1.T.V].F1: Specific data entry selection window (touch screen technology)

OTH.DAT.MAN-[112021.L2.T.V].1When the Hour Glass symbol (ST05) disappears, the National data entry selection window offers the possibility to the driver to select , ... (1) and (2) as indicated in Figure OTH.DAT.MAN-[112021.L2.T.V].F1.

Figure OTH.DAT.MAN-[112021.L2.T.V].F1: National data entry selection window (touch screen technology)

OTH.DAT.MAN-[2230.L2.T.V].1When the Hour Glass symbol (ST05) disappears, the National data entry selection window offers the possibility to the driver to select NTC A , NTC B (1) and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L2.T.V].F1.

Figure OTH.DAT.MAN-[2230.L2.T.V].F1: Specific data entry selection window (touch screen technology)

OTH.DAT.MAN-[112021.L0N1.S.V].1When the Hour Glass symbol (ST05) disappears, the National data entry selection window offers the possibility to the driver to select , ... (1) and (2) as indicated in Figure OTH.DAT.MAN-[112021.L0N1.S.V].F1.

Figure OTH.DAT.MAN-[112021.L0N1.S.V].F1: National data entry selection window (soft key technology)

OTH.DAT.MAN-[2230.L0N1.S.V].1When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select ATO, NTC A , NTC B (1) and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L0N1.S.V].F1.

Figure OTH.DAT.MAN-[2230.L0N1.S.V].F1: Specific data entry selection window (soft key technology)

OTH.DAT.MAN-[112021.L2.S.V].1When the Hour Glass symbol (ST05) disappears, the National data entry selection window offers the possibility to the driver to select , ... (1) and (2) as indicated in Figure OTH.DAT.MAN-[112021.L2.S.V].F1.

Figure OTH.DAT.MAN-[112021.L2.S.V].F1: National data entry selection window (soft key technology)

OTH.DAT.MAN-[2230.L2.S.V].1When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select NTC A , NTC B (1) and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L2.S.V].F1.

Figure OTH.DAT.MAN-[2230.L2.S.V].F1: Specific data entry selection window (soft key technology)

OTH.DAT.MAN-[V].5To enter the data for a specific NTC system, the driver shall press the specific NTC button.

Each specific NTC button is enabled when:

1. The train is at standstill AND
2. The Driver ID is valid AND
3. The ERTMS/ETCS level is valid AND
4. The mode is SB/FS/LS/SR/OS/UN/SN AND
5. The specific signal from the NTC system is received.

OTH.DAT.MAN-[V].6The driver can skip the data entry/validation process of all the NTCs supported by STM by pressing the button. In this case, the ETCS data entry process continues.

The End of data entry button is enabled when:

1. The train is at standstill AND
2. The Driver ID is valid AND
3. The ERTMS/ETCS level is valid AND
4. The mode is SB/FS/LS/SR/OS/UN/SN

To abort the full train data entry procedure, the driver shall press the button.

OTH.DAT.MAN-[V].7The driver can initiate the entry of NTC A data once the NTC A data window(s) is displayed. Note: NTC A is written to indicate the specific NTC selected by the driver in the National data entry selection window.

OTH.DAT.MAN-[T.V].7To entry NTC data, the driver shall select the input field to enter by pressing on it (1), then enter or re-enter/revalidate the data using the associated keyboard (2) and finally confirm it by pressing the button (3) as indicated in Figure OTH.DAT.MAN-[T.V].F7.

Figure OTH.DAT.MAN-[T.V].F7: NTC A data window (touch screen technology)

OTH.DAT.MAN-[S.V].7To entry NTC data, the driver shall select the input field to enter by using the and scrolls buttons (1), then enter or re-enter/revalidate the data using the associated keyboard (2) and finally confirm it by pressing the button (3) as indicated in Figure OTH.DAT.MAN-[S.V].F7.

Figure OTH.DAT.MAN-[S.V].F7: NTC A data window (soft key technology)

OTH.DAT.MAN-[T.V].8After the NTC data entry has been completed, the NTC A data validation window is displayed. The driver has to validate or not validate the values of the input fields for NTC A data by pressing either the or options (1) and then confirming the answer (2), as indicated in Figure OTH.DAT.MAN-[T.V].F8.

Figure OTH.DAT.MAN-[T.V].F8: NTC A data validation window (touch screen technology)

OTH.DAT.MAN-[S.V].8After the NTC data entry has been completed, the NTC A data validation window is displayed. The driver has to validate or not the values of the input fields for NTC A data by pressing either the or options (1) and then confirming the answer by pressing (2), as indicated in Figure OTH.DAT.MAN-[S.V].F8.

Figure OTH.DAT.MAN-[S.V].F8: NTC A data validation window (soft key technology)

OTH.DAT.MAN-[V].8After validating the NTC A data, the Hour Glass symbol (ST05) is displayed to indicate to the driver that the ETCS on-board awaits an answer from all the STM supporting NTC A.

In case of the NTC entry data request received from the STM supporting NTC A, the NTC A data window(s) is displayed to allow the driver to complete the NTC A data entry.

OTH.DAT.MAN-[V].9Otherwise, the NTC data entry selection window is displayed. The driver can enter other NTC data by pressing the button or the driver can end the National data entry selection process by pressing the button.

OTH.DAT.MAN-[2230.L0N1.T.V].2When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select, ATO (1), NTC A , NTC B and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L0N1.T.V].F2.

Figure OTH.DAT.MAN-[2230.L0N1.T.V].F2: Specific data entry selection window (touch screen technology)

OTH.DAT.MAN-[2230.L2.T.V].2When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select, ATO (1), NTC A , NTC B and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L2.T.V].F2.

Figure OTH.DAT.MAN-[2230.L2.T.V].F2: Specific data entry selection window (touch screen technology)

OTH.DAT.MAN-[2230.L0N1.S.V].2When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select ATO , (1), NTC A , NTC B and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L0N1.S.V].F2.

Figure OTH.DAT.MAN-[2230.L0N1.S.V].F2: Specific data entry selection window (soft key technology)

OTH.DAT.MAN-[2230.L2.S.V].2When the Hour Glass symbol (ST05) disappears, the Specific data entry selection window offers the possibility to the driver to select ATO , (1), NTC A , NTC B and End of data entry (2) as indicated in Figure OTH.DAT.MAN-[2230.L2.S.V].F2.

Figure OTH.DAT.MAN-[2230.L2.S.V].F2: Specific data entry selection window (soft key technology)

OTH.DAT.MAN-[2230.V].2To enter the data for the ATO system, the driver shall press the ATO button.

The ATO button is enabled when:

1. The train is at standstill AND
2. The Driver ID is valid AND
3. The ERTMS/ETCS level is valid AND
4. The mode is SB/AD/FS/LS/SR/OS/UN/SN AND
5. The specific signal from the ATO on-board is received.

OTH.DAT.MAN-[2230.V].3The driver can skip the data entry/validation process of the ATO by pressing the End of data entry button. In this case, the ETCS data entry process continues.

The End of data entry button is enabled when:

1. The train is at standstill AND
2. The Driver ID is valid AND
3. The ERTMS/ETCS level is valid AND
4. The mode is SB/AD/FS/LS/SR/OS/UN/SN

To abort the full train data entry procedure, the driver shall press the button.

OTH.DAT.MAN-[2230.V].4If the driver chooses to skip the Specific ATO Data Entry while in the Specific ATO Data Entry window, the ATO Data is considered invalid in the ETCS-OB until the Specific ATO Data Entry process is initiated by the driver and validated.

Conversely, the ATO-OB may not require Specific ATO Data. In that case, the ATO-OB does not request Specific ATO Data and the Specific ATO Data Entry is automatically skipped by the ETCS-OB.

OTH.DAT.MAN-[2230.V].5The Specific ATO Data Entry is also aborted if either:

1. The communication between the ETCS-OB and the ATO-OB times out after a predefined value;
2. The Train Data Entry procedure is aborted by the ETCS-OB for reasons not related to the ATO-OB interface (e.g. the cab deactivation...)

OTH.DAT.MAN-[2230.V].6In case of the ATO entry data request received from the ATO on-board, the ATO data window is displayed to allow the driver to complete the ATO data entry.

The driver can initiate the entry of ATO specific data once the ATO data window is displayed.

OTH.DAT.MAN-[2230.T.V].1To enter ATO data, the driver shall select the input field to enter by pressing on it (1), then enter or re-enter/revalidate the data using the associated keyboard (2) and finally confirm it by pressing the Yes button (3) as indicated in Figure OTH.DAT.MAN-[2230.T.V].F1.

Figure OTH.DAT.MAN-[2230.T.V].F1: ATO data window (touch screen technology)

OTH.DAT.MAN-[2230.S.V].1To enter ATO data, the driver shall select the input field to enter by using the and scrolls buttons (1), then enter or re-enter/revalidate the data using the associated keyboard (2) and finally confirm it by pressing the button (3) as indicated in Figure OTH.DAT.MAN-[2230.S.V].F1.

Figure OTH.DAT.MAN-[2230.S.V].F1: ATO data window (soft key technology)

OTH.DAT.MAN-[2230.T.V].2After the ATO data entry has been completed, the NTC A data validation window is displayed. The driver has to validate or not validate the values of the input fields for NTC A data by pressing either the Yes or No options (1) and then confirming the answer (2), as indicated in Figure OTH.DAT.MAN-[2230.T.V].F2.

Figure OTH.DAT.MAN-[2230.T.V].F2: ATO data validation window (touch screen technology)

OTH.DAT.MAN-[2230.S.V].2After the ATO data entry has been completed, the ATO data validation window is displayed. The driver has to validate or not the values of the input fields for ATO data by pressing either the Yes or No options (1) and then confirming the answer by pressing (2), as indicated in Figure OTH.DAT.MAN-[2230.S.V].F2.

Figure OTH.DAT.MAN-[2230.S.V].F2: ATO data validation window (soft key technology)

OTH.DAT.MAN-[2230.V].7After validating the ATO data, the Hour Glass symbol (ST05) is displayed to indicate to the driver that the ETCS on-board awaits an answer from the ATO on-board.

OTH.DAT.MAN-[2230.V].8Otherwise, the Specific data entry selection window is displayed. The driver can re-enter ATO data by pressing the ATO button or NTC data by pressing the NTC X button or the driver can end the Specific data entry selection process by pressing the End of data entry button.

OTH.DAT.MAN-[2230.V].9If a train movement is detected while the Specific ATO Data Entry is in progress, the ETCS on-board equipment will trigger the brake command. The brake command is consequently released when train is at standstill.

OTH.DAT.MAN-[V].10If an a data entry or validation window is currently displayed when acknowledgement from the driver is required, the data entry/validation process is stopped, the parent window is displayed instead and the driver’s acknowledgement appears.

OTH.DAT.MAN.8After modifying the train data, the driver shall re-enter or re-validate the Train number if it is not valid, see section OTH.ODA.TN Change of Train Running number (TN).

When the Train Data Entry and Train Running Number are completed and validated, the Main window is presented to the driver.

OTH.DAT.MAN-[L2].1If the validated ETCS level is 2, communication with the RBC is established. Once the communication with the RBC is established, the Main window is presented.

OTH.DAT.MAN-[30].2If the safe consist length information is available and as long as the safe consist length in front of the engine, taking into account the side of the active cab which defines the front of the engine, is different from zero:

1. The ERTMS/ETCS on-board equipment shall consider that no valid Train Data is stored on-board
2. The entry, modification and revalidation of Train Data that requires driver validation shall not be possible

### OTH.DAT.EXTChange of train data by ETCS external sources (EXT)

OTH.DAT.EXT.1When the text message “Train data changed” is displayed on the DMI:

1. If the change of train data leads to an application of the brake, when at a standstill, the driver shall acknowledge the brake application as indicated in the following clauses.
2. In all other cases, the driver shall take into account the modified train data.

OTH.DAT.EXT-[L0N1.T].1When a change of train data has led to an application of the brake, the driver is informed about this by the Brake intervention symbol (ST01) (1) and the system status message “Train data changed” (2) as indicated in Figure OTH.DAT.EXT-[L0N1.T].F1.

Figure OTH.DAT.EXT-[L0N1.T].F1: Brake intervention when Train Data is changed (touch screen technology)

OTH.DAT.EXT-[L2.T].1When a change of train data has led to an application of the brake, the driver is informed about this by the Brake intervention symbol (ST01) (1) and the system status message “Train data changed” (2) as indicated in Figure OTH.DAT.EXT-[L2.T].F1.

Figure OTH.DAT.EXT-[L2.T].F1: Brake intervention when Train Data is changed (touch screen technology)

OTH.DAT.EXT-[L0N1.S].1When a change of train data has led to an application of the brake, the driver is informed about this by the Brake intervention symbol (ST01) (1) and the system status message “Train data changed” (2) as indicated in Figure OTH.DAT.EXT-[L0N1.S].F1.

Figure OTH.DAT.EXT-[L0N1.S].F1: Brake intervention when Train Data is changed (soft key technology)

OTH.DAT.EXT-[L2.S].1When a change of train data has led to an application of the brake, the driver is informed about this by the Brake intervention symbol (ST01) (1) and the system status message “Train data changed” (2) as indicated in Figure OTH.DAT.EXT-[L2.S].F1.

Figure OTH.DAT.EXT-[L2.S].F1: Brake intervention when Train Data is changed (soft key technology)

OTH.DAT.EXT-[L0N1.T].2When the train is at standstill, the driver shall acknowledge the brake application by pressing the button with the flashing frame as indicated in the Figure BRK-[L0N1.T].F1.

Figure OTH.DAT.EXT-[L0N1.T].F1: Brake intervention to be acknowledged (touch screen technology)

OTH.DAT.EXT-[L2.T].2When the train is at standstill, the driver shall acknowledge the brake command by pressing the button with the flashing frame as indicated in the Figure BRK-[L2.T].F1.

Figure OTH.DAT.EXT-[L2.T].F2: Brake intervention to be acknowledged (touch screen technology)

OTH.DAT.EXT-[L0N1.S].2When the train is at standstill, the driver shall acknowledge the brake command by pressing the button with the flashing frame as indicated in the Figure BRK-[L0N1.S].F1.

Figure OTH.DAT.EXT-[L0N1.S].F2: Brake intervention to be acknowledged (soft key technology)

OTH.DAT.EXT-[L2.S].2When the train is at standstill, the driver shall acknowledges the brake command by pressing the button with the flashing frame as indicated in the Figure BRK-[L2.S].F1.

Figure OTH.DAT.EXT-[L2.S].F2: Brake intervention to be acknowledged (soft key technology)

OTH.DAT.EXT.2After acknowledging the brake application, the driver shall:

1. Modify and/or validate the train data, if requested to by the ETCS on-board system (see section OTH.DAT.MAN Manual change of train data (MAN)) AND,
2. Take into account the modified train data.

OTH.DAT.EXT-[L12].1If a change in train data leads to an application of the brake in level 1 and level 2 if no new MA is received, the driver cannot pass the EOA until the signaller authorises it (see section OVR - Authorising the passing of an EOA (OVR)).

## OTH.ODAChanging other data (ODA)

OTH.ODA-[N].1If a change is required, the driver shall enter/modify and validate the driver identification, the train running number, the radio network identification and the RBC identification/phone number.

OTH.ODA.1To change/modify the driver identification, train number and radio information data, the driver shall access the Main window.

OTH.ODA-[L0N1.T].1To enter the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L0N1.T].F2.

Figure MAIN-[L0N1.T].F2: Main button on Default window (touch screen technology)

OTH.ODA-[L2.T].1To enter the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L2.T].F2.

Figure MAIN-[L2.T].F2: Main button on Default window (touch screen technology)

OTH.ODA-[L0N1.S].1To enter the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L0N1.S].F2.

Figure MAIN-[L0N1.S].F2: Main button on Default window (soft key technology)

OTH.ODA-[L2.S].1To enter the Main window, the driver shall press the button on the Default window of the DMI as indicated in Figure MAIN-[L2.S].F2.

Figure MAIN-[L2.S].F2: Main button on Default window (soft key technology)

OTH.ODA.2As a result, the Main window is presented to the driver.

The steps to follow to modify the Driver ID, TRN and Radio data are collected in the following sections.

### OTH.ODA.DRVChange of driver identification (DRV)

OTH.ODA.DRV-[N].1If a change is required, the driver shall enter, modify and validate the driver identification while at standstill or, if allowed by national value, while running.

OTH.ODA.DRV.1The modification of the driver identification data is carried out from the Main window, the steps to access this window are explicated at the beginning of this section, OTH.ODA Changing other data (ODA).

OTH.ODA.DRV-[B3241.L0N1.T].1To re-enter or re-validate the Driver ID data, the driver shall press the button in the Main window, as indicated in Figure OTH.ODA.DRV-[B3241.L0N1.T].F1.

Figure OTH.ODA.DRV-[B3241.L0N1.T].F1: Driver ID button on Main window (touch screen technology)

OTH.ODA.DRV-[B3241.L2.T].1To re-enter or re-validate the Driver ID data, the driver shall press the button in the Main window, as indicated in Figure OTH.ODA.DRV-[B3241.L2.T].F1.

Figure OTH.ODA.DRV-[B3241.L2.T].F1: Driver ID button on Main window (touch screen technology)

OTH.ODA.DRV-[B3241.L0N1.S].2To re-enter or re-validate the Driver ID data, the driver shall press the button associated to the Driver ID label in the Main window, as indicated in Figure OTH.ODA.DRV-[B3241.L0N1.S].F1.

Figure OTH.ODA.DRV-[B3241.L0N1.S].F1: Driver ID button on Main window (soft key technology)

OTH.ODA.DRV-[B3241.L2.S].1To re-enter or re-validate the Driver ID data, the driver shall press the button associated to the Driver ID label in the Main window, as indicated in Figure OTH.ODA.DRV-[B3241.L2.S].F1.

Figure OTH.ODA.DRV-[B3241.L2.S].F1: Driver ID button on Main window (soft key technology)

OTH.ODA.DRV-[B3M1.L0N1.T].1To re-enter or re-validate the Driver ID data, the driver shall press the button in the Main window, as indicated in Figure OTH.ODA.DRV-[B3M1.L0N1.T].F1.

Figure OTH.ODA.DRV-[B3M1.L0N1.T].F1: Driver ID button on Main window (touch screen technology)

OTH.ODA.DRV-[B3M1.L23.T].1To re-enter or re-validate the Driver ID data, the driver shall press the button in the Main window, as indicated in Figure OTH.ODA.DRV-[B3M1.L23.T].F1.

Figure OTH.ODA.DRV-[B3M1.L23.T].F1: Driver ID button on Main window (touch screen technology)

OTH.ODA.DRV-[B3M1.L0N1.S].1To re-enter or re-validate the Driver ID data, the driver shall press the button associated to the Driver ID label in the Main window, as indicated in Figure OTH.ODA.DRV-[B3M1.L0N1.S].F1.

Figure OTH.ODA.DRV-[B3M1.L0N1.S].F1: Driver ID button on Main window (soft key technology)

OTH.ODA.DRV-[B3M1.L23.S].1To re-enter or re-validate the Driver ID data, the driver shall press the button associated to the Driver ID label in the Main window, as indicated in Figure OTH.ODA.DRV-[B3M1.L23.S].F1.

Figure OTH.ODA.DRV-[B3M1.L23.S].F1: Driver ID button on Main window (soft key technology)

OTH.ODA.DRV.2The Driver ID button is enabled to change the Driver ID data when:

1. The train is at standstill AND mode is SB AND the Driver ID, train data, ETCS level are valid OR
2. The train is at standstill AND mode is SH, FS, LS, SR, OS, NL, UN, SN.

OTH.ODA.DRV-[22].1The Driver ID button is also enabled in AD mode.

OTH.ODA.DRV-[30].1The Driver ID button is also enabled in AD and SM mode.

OTH.ODA.DRV-[N].2If allowed by a National value, the driver shall also have the possibility to modify the Driver ID while the train is running in modes SH/FS/LS/SR/OS/NL/UN/SN.

OTH.ODA.DRV-[22.N].1If allowed by a National value, the driver may also modify the Driver ID while running in AD mode.

OTH.ODA.DRV-[30].1If allowed by a National value, the driver may also modify the Driver ID while running in AD and SM mode.

OTH.ODA.DRV-[L0N1.T].2The driver shall enter the Driver ID in the Driver ID window in the input field (1) and then, confirm it by pressing data field itself (2) as indicated in Figure DRV-[L0N1.T].F2.

Figure DRV-[L0N1.T].F2: Driver ID window (touch screen technology)

OTH.ODA.DRV-[L2.T].2The driver shall enter the Driver ID in the Driver ID window in the input field (1) and then, confirm it by pressing data field itself (2) as indicated in Figure DRV-[L2.T].F1 .

Figure DRV-[L2.T].F1: Driver ID window (touch screen technology)

OTH.ODA.DRV-[L0N1.S].2The driver shall enter the Driver ID in the Driver ID window in the input field (1) and then, confirm the Driver ID by pressing the button (2) as indicated in Figure DRV-[L0N1.S].F2.

Figure DRV-[L0N1.S].F2: Driver ID window (soft key technology)

OTH.ODA.DRV-[L2.S].2The driver shall enter the Driver ID in the Driver ID window in the input field (1) and then, confirm the Driver ID by pressing the button (2) as indicated in Figure DRV-[L2.S].F1.

Figure DRV-[L2.S].F1: Driver ID window (soft key technology)

OTH.ODA.DRV.3When the Driver ID data has been entered and validated, the Main window is presented to the Driver.

### OTH.ODA.TNChange of Train Running number (TN)

OTH.ODA.TN-[N].1If a change is required, the driver shall enter/modify and validate the train running number.

OTH.ODA.TN.1The modification of the train number data is carried out from the Main window, the steps to access this window are explicated at the beginning of this section, OTH.ODA Changing other data (ODA).

OTH.ODA.TN-[B3241.L0N1.T].1To re-enter or re-validate the Train running number, the driver shall press the button in the Main window as indicated in Figure OTH.ODA.OTH.ODA.TN-[B3241.L0N1.T].F1.

Figure OTH.ODA.TN-[B3241.L0N1.T].F1: Train running number button on Main window (touch screen technology)

OTH.ODA.TN-[B3241.L2.T].1To re-enter or re-validate the Train running number, the driver shall press the button in the Main window as indicated in Figure OTH.ODA.TN-[B3241.L2.T].F1.

Figure OTH.ODA.TN-[B3241.L2.T].F1: Train running number button on Main window (touch screen technology)

OTH.ODA.TN-[B3241.L0N1.S].1To re-enter or re-validate the Train running number, the driver shall press the button associated to the Train running number label in the Main window as indicated in Figure OTH.ODA.OTH.ODA.TN-[B3241.L0N1.S].F1.

Figure OTH.ODA.TN-[B3241.L0N1.S].F1: Train running number button on Main window (soft key technology)

OTH.ODA.TN-[B3241.L2.S].1To re-enter or re-validate the Train running number, the driver shall press the button associated to the Train running number label in the Main window as indicated in Figure OTH.ODA.TN-[B3241.L2.S].F1.

Figure OTH.ODA.TN-[B3241.L2.S].F1: Train running number button on Main window (soft key technology)

OTH.ODA.TN-[B3M1.L0N1.T].1To re-enter or re-validate the Train running number, the driver shall press the button in the Main window as indicated in Figure OTH.ODA.TN-[B3M1.L0N1.T].F1.

Figure OTH.ODA.TN-[B3M1.L0N1.T].F1: Train running number button on Main window (touch screen technology)

OTH.ODA.TN-[B3M1.L2.T].1To re-enter or re-validate the Train running number, the driver shall press the button in the Main window as indicated in Figure OTH.ODA.TN-[B3M1.L2.T].F1.

Figure OTH.ODA.TN-[B3M1.L2.T].F1: Train running number button on Main window (touch screen technology)

OTH.ODA.TN-[B3M1.L0N1.S].1To re-enter or re-validate the Train running number, the driver shall press the button associated to the Train running number label in the Main window as indicated in Figure OTH.ODA.TN-[B3M1.L0N1.S].F1.

Figure OTH.ODA.TN-[B3M1.L0N1.S].F1: Train running number button on Main window (soft key technology)

OTH.ODA.TN-[B3M1.L2.S].1To re-enter or re-validate the Train running number, the driver shall press the button associated to the Train running number label in the Main window as indicated in Figure OTH.ODA.TN-[B3M1.L2.S].F1.

Figure OTH.ODA.TN-[B3M1.L2.S].F1: Train running number button on Main window (soft key technology)

OTH.ODA.TN.2The Train running number button is enabled to change the Train number data when:

1. The train is at standstill AND, Mode is SB AND, the Driver ID and ETCS level are valid OR,
2. The mode is FS/LS/SR/OS/NL/UN/SN.

OTH.ODA.TN-[22].1The Train running number button is also enabled in AD mode.

OTH.ODA.TN-[30].1The Train running number button is also enable in AD and SM mode.

OTH.ODA.TN-[L0N1.T].2The driver shall enter the Train running number data in the available input field using the associated keyboard (1) and confirm it by pressing the input field itself (2) as indicated in Figure OTH.ODA.TN-[L0N1.T].F2.

Figure OTH.ODA.TN-[L0N1.T].F2: Train running number window (touch screen technology)

OTH.ODA.TN-[L2.T].2The driver shall enter the Train running number data in the available input field using the associated keyboard (1) and confirm it by pressing the input field itself (2) as indicated in Figure TN-[L2.T].F1.

Figure TN-[L2.T].F1: Train running number window (touch screen technology)

OTH.ODA.TN-[L0N1.S].2The driver shall enter the Train running number data in the available input field using the buttons of the associated keyboard (1) and confirm it by pressing the button (2) as indicated in Figure OTH.ODA.TN-[L0N1.S].F2.

Figure OTH.ODA.TN-[L0N1.S].F2: Train running number window (soft key technology)

OTH.ODA.TN-[L2.S].2The driver shall enter the Train running number data in the available input field using the buttons of the associated keyboard (1) and confirm it by pressing the button (2) as indicated in Figure TN-[L2.S].F1.

Figure TN-[L2.S].F1: Train running number window (soft key technology)

OTH.ODA.TN.3Once the Train number data has been entered and validated, the Main window is presented to the driver.

OTH.ODA.TN-[2230].1If the Train number is changed by the driver for a train equipped with an active ATO, the ATO-OB shall delete any stored Journey Profile information received from the ATO-TS and request a new Journey Profile.

OTH.ODA.TN.4In addition to driver input, the RBC or other ETCS external sources can change the Train running number while the train is running.

OTH.ODA.TN-[2230].2If the Train number becomes invalid, the ATO-OB shall terminate the communication session with the ATO-TS.

### OTH.ODA.RADChange of Radio information (RAD)

OTH.ODA.RAD-[N].1The driver shall enter/modify and validate the radio network identification and the RBC identification/phone number when required.

OTH.ODA.RAD-[B3M1.L23].1The driver can re-enter the radio information through the level button of the Main window. Once the ETCS level is re-entered or revalidated and it is ETCS level 2 or 3, the option to enter or revalidate the radio data is presented to the driver.

OTH.ODA.RAD-[B3241].1The modification of the radio information data is carried out from the Main window, the steps to access this window are explicated at the beginning of this section, OTH.ODA Changing other data (ODA).

OTH.ODA.RAD-[B3241.11202122.L2.T].1To re-enter or re-validate the Radio information, the driver shall press the button in the Main window as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F1.

Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F1: Radio data button on Main window (touch screen technology)

OTH.ODA.RAD-[30.L2.T].1To re-enter or re-validate the Radio information, the driver shall press the Radio data button in the Main window as indicated in Figure OTH.ODA.RAD-[30.L2.T].F1.

Figure OTH.ODA.RAD-[30.L2.T].F1: Radio data button on Main window (touch screen technology)

OTH.ODA.RAD-[B3241.11202122.L2.S].1To re-enter or re-validate the Radio information, the driver shall press the button associated to the Radio data label on the Main window as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F1.

Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F1: Radio data button on Main window (soft key technology)

OTH.ODA.RAD-[30.L2.S].1To re-enter or re-validate the Radio information, the driver shall first press the button associated with the "..." label in the Main window to display the last two options and then press the button associated to the Radio data label on the Main window as indicated in Figure OTH.ODA.RAD-[30.L2.S].F1.

Figure OTH.ODA.RAD-[30.L2.S].F1: Radio data button on Main window (soft key technology)

OTH.ODA.RAD-[B3241.112021.L2].1The Radio data button is enabled to change the radio data when:

1. The train is at standstill AND,
2. The Driver ID is valid AND,
3. The ETCS level is valid AND,
4. The mode is SB, FS, LS, SR, OS, NL, PT, UN, SN.

OTH.ODA.RAD-[22.L2].1The Radio data button is enabled to change the radio data when:

1. The train is at standstill AND,
2. The Driver ID is valid AND,
3. The ETCS level is valid AND,
4. The mode is SB, FS, AD, LS, SR, OS, NL, PT, UN, SN.

OTH.ODA.RAD-[30.L2].1The Radio data button is enabled to change the radio data when:

1. The train is at standstill AND,
2. The Driver ID is valid AND,
3. The ETCS level is valid AND,
4. The mode is SB, FS, AD, SM, LS, SR, OS, NL, PT, UN, SN.

OTH.ODA.RAD-[B3241.112021.L0N1].1In level NTC and ETCS level 0 or 1, the Radio Data button on the Main window is enabled and the driver could introduce the Radio Network ID when:

1. The train is at standstill AND,
2. The Driver ID is valid AND,
3. The mode is SB/FS/LS/SR/OS/NL/PT/UN/SN AND,
4. The ETCS level is valid.

To introduce other Radio Information, the ETCS level entered or revalidated must be ETCS level 2.

OTH.ODA.RAD-[2230.L0N1].1In level NTC and ETCS level 0 or 1, the Radio Data button on the Main window is enabled and the driver could introduce the Radio Network ID when:

1. The train is at standstill AND,
2. The Driver ID is valid AND,
3. The mode is SB/FS/AD/LS/SR/OS/NL/PT/UN/SN AND,
4. The ETCS level is valid.

To introduce other Radio Information, the ETCS level entered or revalidated must be ETCS level 2.

OTH.ODA.RAD-[30.L2.T].2To re-enter, re-validate or change the radio network type, the driver shall press the Radio Network Type button on the Radio data window, as indicated in Figure OTH.ODA.RAD-[30.L2.T].F2. Any ongoing communication session terminates with this action.

Figure OTH.ODA.RAD-[30.L2.T].F2: Radio data window (touch screen technology)

OTH.ODA.RAD-[30.L2.S].2To re-enter, re-validate or change the radio network type, the driver shall press the button associated with the Radio Network Type label on the Radio data window, as indicated in Figure OTH.ODA.RAD-[30.L2.S].F2. Any ongoing communication session terminates with this action.

Figure OTH.ODA.RAD-[30.L2.S].F2: Radio data window (soft key technology)

OTH.ODA.RAD-[30.L2.T.N].1The driver shall select one of the radio network types (1) and then confirm it by pressing on the input field itself (2) as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F1.

Figure OTH.ODA.RAD-[30.L2.T.N].F1: Radio network type window (touch screen technology)

OTH.ODA.RAD-[30.L2.S.N].1The driver shall select one of the radio network types by pressing on the button associated with the corresponding label (1) and then confirm the selection by pressing the button (2) as indicated in Figure OTH.ODA.RAD-[30.L2.S.N].F1.

Figure OTH.ODA.RAD-[30.L2.S.N].F1: Radio network type window (soft key technology)

OTH.ODA.RAD-[30.L2.N].1If the FRMCS is installed on board and the driver selects FRMCS or FRMCS+GSM-R, and the FRMCS on-board is not registered to the FRMCS Radio Network, the DMI shall display the text message “FRMCS network registration failed” in area E to inform the driver that the FRMCS network registration has failed.

OTH.ODA.RAD-[30.L2.V].1If GSM-R is not installed on-board along the FRMCS, the Main window is presented to the driver and the text message disappears as soon as any button in this window is selected.

OTH.ODA.RAD-[30.L2.V].2If GSM-R is also installed on-board, the driver is presented again with the Radio Data window, and the text message disappears as soon as the driver elects to perform the mission with only one radio system by selecting the button.

OTH.ODA.RAD-[30.L2].2If the Network Type is selected and confirmed, and no registration failure message is displayed, the driver is presented again with the Radio Data window.

OTH.ODA.RAD-[B3241.11202122.L2.T].2To re-enter, re-validate or change the Radio network ID data, the driver shall press the button on the Radio data window, as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F2. Any ongoing communication session terminates with this action.

The button is a delay-type button, meaning that the driver must keep pressing during 2 seconds to be considered by the DMI. If the button is pressed by the driver for less than the 2 seconds, no valid request to select the Radio Network ID shall be considered by the onboard.

Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F2: Radio data window (touch screen technology)

OTH.ODA.RAD-[30.L2.T.N].2To re-enter, re-validate or change the GSM-R network ID data, in case the Network Type is FRMCS or FRMCS+GSM-R, the driver shall press the button on the Radio data window, as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F2. Any ongoing communication session terminates with this action.

The button is a delay-type button, meaning that the driver must keep pressing during 2 seconds to be considered by the DMI. If the button is pressed by the driver for less than the 2 seconds, no valid request to select the GSM-R Network ID shall be considered by the onboard.

Figure OTH.ODA.RAD-[30.L2.T.N].F2: Radio data window (touch screen technology)

OTH.ODA.RAD-[B3241.11202122.L2.S].2To re-enter, re-validate or change the Radio network ID data, the driver shall press the button associated to the Radio Network ID label on the Radio data window, as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F2. Any ongoing communication session terminates with this action.

The button is a delay-type button, meaning that the driver must keep pressing during 2 seconds to be considered by the DMI. If the button is pressed by the driver for less than the 2 seconds, no valid request to select the Radio Network ID shall be considered by the onboard.

Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F2: Radio data window (soft key technology)

OTH.ODA.RAD-[30.L2.S.N].2To re-enter, re-validate or change the GSM-R network ID data, in case the Network Type is FRMCS or FRMCS+GSM-R, the driver shall press the button associated to the label on the Radio data window, as indicated in Figure OTH.ODA.RAD-[30.L2.S.N].F2. Any ongoing communication session terminates with this action.

The button is a delay-type button, meaning that the driver must keep pressing during 2 seconds to be considered by the DMI. If the button is pressed by the driver for less than the 2 seconds, no valid request to select the GSM-R Network ID shall be considered by the onboard.

Figure OTH.ODA.RAD-[30.L2.S.N].F2: Radio data window (soft key technology)

OTH.ODA.RAD-[B3241.11202122.L2].1The Radio data window is presented to the driver with all buttons disabled and the Hour Glass symbol (ST05) displayed on the window indicating that the list of available and allowed Radio Networks is being acquired.

OTH.ODA.RAD-[30.L2].3The Radio data window is presented to the driver with all buttons disabled and the Hour Glass symbol (ST05) displayed on the window indicating that the list of available and allowed GSM-R Networks is being acquired.

OTH.ODA.RAD-[B3241.11202122.L2].2The text message “Radio network registration failed” is displayed in area E, if the list of available Radio networks shows there are no Radio networks available. Consequently, the radio data entry finishes, and the Main window is shown to the driver again.

When this text message appears, the driver shall enter the radio network identification.

OTH.ODA.RAD-[30.L2].4The text message “GSM-R network registration failed” is displayed in area E if the list of available GSM-R networks shows there are no GSM-R networks available.

When this text message appears, the driver shall enter the GSM-R network identification.

OTH.ODA.RAD-[30.L2.N].2In case the Network Type is FRMCS+GSM-R, the driver is presented with the Radio data window again and the text message disappears as soon as the driver selects Mission with one radio system.

OTH.ODA.RAD-[30.L2.N].3In case the Network Type is GSM-R, the Main window is presented to the driver and the text message disappears as soon as any button in this window is selected.

OTH.ODA.RAD-[B3241.11202122.L2].3Otherwise, the Radio network ID window is presented to the driver with the list of available networks.

OTH.ODA.RAD-[30.L2].5Otherwise, the GSM-R network ID window is presented to the driver with the list of available networks.

OTH.ODA.RAD-[B3241.11202122.L2.T].3The driver shall select one of the available and allowed radio networks shown in the window (1) and then confirm the selection by pressing on the input field itself (2) as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F3.

Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F3: Radio network ID window (touch screen technology)

OTH.ODA.RAD-[30.L2.T].3The driver shall select one of the available and allowed radio networks shown in the window (1) and then confirm the selection by pressing on the input field itself (2) as indicated in Figure OTH.ODA.RAD-[30.L2.T].F3.

Figure OTH.ODA.RAD-[30.L2.T].F3: GSM-R network ID window (touch screen technology)

OTH.ODA.RAD-[B3241.11202122.L2.S].3The driver shall select one of the available and allowed Networks shown in the window (1) and then confirm the selection by pressing on the button (2) as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F3.

Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F3: Radio network ID window (soft key technology)

OTH.ODA.RAD-[30.L2.S].3The driver shall select one of the available and allowed Networks shown in the window (1) and then confirm the selection by pressing on the button (2) as indicated in Figure OTH.ODA.RAD-[30.L2.S].F3.

Figure OTH.ODA.RAD-[30.L2.S].F3: GSM-R network ID window (soft key technology)

OTH.ODA.RAD-[B3241.11202122.L2].4Once the Radio Network ID is selected, the Radio data window is presented to the driver with all the buttons disabled and the Hour Glass symbol (ST05) displayed, to indicate that the registration to the Radio Network is being processed.

OTH.ODA.RAD-[30.L2].6Once the GSM-R Network ID is selected, the Radio data window is presented to the driver with all the buttons disabled and the Hour Glass symbol (ST05) is displayed to indicate that the registration to the GSM-R Network is being progressed.

OTH.ODA.RAD-[B3241.11202122.L2].5The buttons of the Radio data window are enabled again when at least one Mobile Terminal is registered to the new Radio Network, offering the following options for the RBC-ID/phone number to the driver:

1. To use the last stored RBC-ID/phone number (Contact last RBC button).
2. To use the EIRENE short number (trackside call routing function) (Use short number button).
3. To Enter or re-enter or re-validate the RBC-ID/phone number (Enter RBC data button).

OTH.ODA.RAD-[30.L2].7The buttons on the Radio data window are enabled again when at least one Mobile Terminal is registered to the new GSM-R Network.

OTH.ODA.RAD-[30.L2.N].4The button is enabled when:

1. the Radio Network Type is FRMCS+GSM-R AND,
2. both systems are installed on-board AND,
3. Either one of the systems has not successfully registered, as indicated by the text message GSM-R registration failed or FRMCS registration failed displayed on the DMI.

OTH.ODA.RAD-[30.L2.T.N].3The driver may choose to continue the mission with only one radio system by pressing the button as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F3.

Figure OTH.ODA.RAD-[30.L2.T.N].F3: Radio data window (touch screen technology)

OTH.ODA.RAD-[30.L2.S.N].3The driver may choose to continue the mission with only one radio system by pressing the button with the label as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F3.

Figure OTH.ODA.RAD-[30.L2.T.N].F3: Radio data window (touch screen technology)

OTH.ODA.RAD-[30.L2].8If not already displayed in previous steps, when the button is pressed, the DMI shall display either FRMCS network registration failed or GSM-R network registration failed or both text messages if the applicable system has failed registration to their respective network.

OTH.ODA.RAD-[30.L2.T.N].4To perform the mission with only one radio system, the driver shall select the button (1) and then, confirm it by pressing the input field itself (2) as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F5.

Figure OTH.ODA.RAD-[30.L2.T.N].F5: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[30.L2.S.N].4To perform the mission with only one radio system, the driver shall select the button (1) and then, confirm it by pressing the button (2) as indicated in Figure OTH.ODA.RAD-[30.L2.S.N].F4.

Figure OTH.ODA.RAD-[30.L2.S.N].F4: Mission with one radio system window (soft key technology)

OTH.ODA.RAD-[30.L2.N].5If the driver selects Yes, the driver is presented with the Radio data window.

OTH.ODA.RAD-[30.L2.N].6If the driver selects No, the driver is presented with the Main window.

OTH.ODA.RAD-[30.L2.N].7If both FRMCS and GSM-R radio systems are installed on-board, it shall request the set-up of a safe radio connection according to the following (by priority order):

1. If the stored Radio Network type is FRMCS+GSM-R and if during the SoM the driver has elected to perform the mission with only one radio system, by using either the FRMCS on-board equipment or a GSM-R Mobile Terminal, depending on the radio system to which the registration was successful during the SoM, OR
2. According to the stored Radio Network information (Radio Network type and, if relevant, GSM-R Radio Network ID). If the Radio Network type is FRMCS+GSM-R, the ERTMS/ETCS on-board shall use, if available, the preferred radio system stored when establishing the previous communication session with the RBC.

OTH.ODA.RAD-[30.L2].9The other buttons on the Radio data window are enabled when:

1. At least one radio system, either a GSM-R Mobile Terminal or FRMCS on-board, is installed AND,
2. At least one of the installed radio systems has successfully been registered to the corresponding network(s) AND,
3. If the Network Type is FRMCS+GSM-R and only one of the networks has successfully registered, the driver has elected to perform the mission with only one radio system.

The driver is then offered the following options for the RBC-ID/phone number to the driver:

1. To use the last stored RBC-ID (Contact last RBC button).
2. To use the EIRENE short number (trackside call routing function for GSM-R-equipped on-boards only) (Use short number button).
3. To enter or re-enter or re-validate the RBC-ID number (Enter RBC data button).

OTH.ODA.RAD-[B3241.11202122.L2].6When the driver selects the or button on the Radio data window to use the last stored RBC-ID/phone number or the EIRENE short number, the Main window is presented to the driver with all the buttons disabled and the Hour Glass symbol (ST05) is shown, to indicate that the ETCS on-board awaits an answer from the RBC.

When the session with the RBC is opened, messages between the RBC and the ETCS on-board are exchanged without the intervention of the driver. The driver must wait until the Main window is presented.

OTH.ODA.RAD-[30.L2].10When the driver selects the or button (for GSM-R-equipped on-boards only) on the Radio data window to use the last stored RBC-ID/phone number or the EIRENE short number, the Main window is presented to the driver with all the buttons disabled and the Hour Glass symbol (ST05) is shown, to indicate that the ETCS on-board awaits an answer from the RBC.

The driver must wait until the Main window is presented.

OTH.ODA.RAD-[B3241.L2].1The text message “Trackside not compatible” is displayed in area E, to indicate that the opening of the session has failed due to a non-compatible version. Then, the Main window is presented to the driver to continue with the procedure of data entry.

The train cannot continue in ETCS when this text message appears. The steps that the driver shall follow in this situation are included in section DEG.VER Managing incompatibility system version (VER).

OTH.ODA.RAD-[B3241.11202122.L2.T].4To re-enter, re-validate or change a RBC ID/phone number, the driver shall press the button on the Radio data window as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F4.

Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F4: Radio data window (touch screen technology)

OTH.ODA.RAD-[30.L2.T].4To re-enter, re-validate or change an RBC ID/phone number, the driver shall press the Enter RBC data button on the Radio data window as indicated in Figure OTH.ODA.RAD-[30.L2.T].F4.

Figure OTH.ODA.RAD-[30.L2.T].F4: Radio data window (touch screen technology)

OTH.ODA.RAD-[B3241.11202122.L2.S].4To re-enter, re-validate or change a RBC ID/phone number, the driver shall press the button associated to Enter RBC data label on the Radio data window as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F4.

Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F4: Radio data window (soft key technology)

OTH.ODA.RAD-[30.L2.S].4To re-enter, re-validate or change an RBC ID/phone number, the driver shall press the button associated to Enter RBC data label on the Radio data window as indicated in Figure OTH.ODA.RAD-[30.L2.S].F4.

Figure OTH.ODA.RAD-[30.L2.S].F4: Radio data window (soft key technology)

OTH.ODA.RAD-[L2].2As a result, the RBC data window is presented to the driver.

OTH.ODA.RAD-[B3241.11202122.L2.T].5The driver shall select the input field that the driver wants to enter (RBC ID or RBC phone number) by pressing on it (the top one is selected by default) (1). The driver shall then enter the code using the keyboard (2) and finally confirm it by pressing the button (3) as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F5.

Figure OTH.ODA.RAD-[B3241.11202122.L2.T].F5: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[30.L2.T.N].5If the Radio Network Type is GSM-R, or FRMCS+GSM-R with GSM-R installed on-board, the driver shall select the input field that the driver wants to enter (RBC ID or RBC phone number) by pressing on it (the top one is selected by default) (1). The driver shall then enter the code using the keyboard (2) and finally confirm it by pressing the Yes button (3) as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F5.

Figure OTH.ODA.RAD-[30.L2.T.N].F5: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[30.L2.T.N].6If the Radio Network Type is FRMCS, the driver shall fill the RBC ID (1) by entering the code using the keyboard (2). Finally, the driver shall confirm it by pressing the Yes button (3) as indicated in Figure OTH.ODA.RAD-[30.L2.T.N].F6.

Figure OTH.ODA.RAD-[30.L2.T.N].F6: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[B3241.11202122.L2.S].5The driver shall select the input field that the driver wants to enter (RBC ID or RBC phone number) by using the and buttons (1). The driver shall then enter the code using the keyboard buttons (2) and finally confirm it by pressing the button (3) as indicated in Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F5.

Figure OTH.ODA.RAD-[B3241.11202122.L2.S].F5: RBC ID/ phone number (soft key technology)

OTH.ODA.RAD-[30.L2.S.N].5If the Radio Network Type is GSM-R, or FRMCS+GSM-R with GSM-R installed on-board, the driver shall select the input field that the driver wants to enter (RBC ID or RBC phone number) by pressing on it (the top one is selected by default) (1). The driver shall then enter the code using the keyboard (2) and finally confirm it by pressing the Yes button (3) as indicated in Figure OTH.ODA.RAD-[30.L2.S.N].F5.

Figure OTH.ODA.RAD-[30.L2.S.N].F5: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[30.L2.S.N].6If the Radio Network Type is FRMCS, the driver shall fill the RBC ID (1) by entering the code using the keyboard (2). Finally, the driver shall confirm it by pressing the Yes button (3) as indicated in Figure OTH.ODA.RAD-[30.L2.S.N].F6.

Figure OTH.ODA.RAD-[30.L2.S.N].F6: RBC ID/phone number (touch screen technology)

OTH.ODA.RAD-[B3241.L2].3The Yes button of the RBC data entry complete? question is enabled if all input fields contain a value.

OTH.ODA.RAD-[B3241.L2].4Once the RBC ID/phone number is entered or re-entered/revalidated, the Main window is presented to the driver with all buttons disabled and the Hour Glass symbol (ST05) is shown to indicate that the ETCS on-board awaits an answer from the RBC.

OTH.ODA.RAD-[B3241.L2].5Whether the RBC session opening is successful or not, the driver does not act until the Main window is reached again and the buttons are enabled. The text message “Trackside not compatible” is displayed if the opening of the session is not successful as already mentioned above.

The train cannot continue in ETCS when this text message appears. The steps that the driver shall follow in this situation are included in section DEG.VER Managing incompatibility system version (VER).

OTH.ODA.RAD-[B3241.L2].6When the Radio data has been entered and validated, and the session with RBC is opened, the Main window is presented.

OTH.ODA.RAD-[B3241.L2].7Additionally, the driver can change the radio data after selecting ETCS level 2.

## OTH.ADHChanging of adhesion factor (ADH)

OTH.ADH-[N].1The adhesion factor is used to adjust the emergency braking of the train.

If the national value allows the driver to select ‘Slippery rail’, the driver may do so when the adhesion conditions are poor or when informed by the signaller. If the driver is not informed by the signaller before selecting ‘Slippery rail’, the driver shall inform the signaller.

When a signaller is informed about poor adhesion conditions, the driver shall activate the ETCS reduced adhesion function, where possible, and if this is not possible he/she shall take measures as prescribed by the IM, until normal operation is restored.

OTH.ADH-[L12.N].1When the value of the adhesion factor is slippery rail, the Adhesion Factor Slippery Rail symbol (ST02) is displayed and the driver shall apply non-harmonised rules.

ST02: Adhesion factor slippery rail

OTH.ADH-[L1.T.N].1When the value of the adhesion factor is slippery rail, the driver is informed about this by the Adhesion factor slippery rail symbol (ST02) as indicated in Figure OTH.ADH-[L1.T.N].F1.

Figure OTH.ADH-[L1.T.N].F1: Adhesion Factor Splippery rail (touch screen technology)

OTH.ADH-[L2.T.N].1When the value of the adhesion factor is slippery rail, the driver is informed about this by the Adhesion factor slippery rail symbol (ST02) as indicated in Figure OTH.ADH-[L2.T].F1.

Figure OTH.ADH-[L2.T].F1: Adhesion Factor Slippery rail (touch screen technology)

OTH.ADH-[L1.S.N].1When the value of the adhesion factor is slippery rail, the driver is informed about this by the Adhesion factor slippery rail symbol (ST02) as indicated in Figure OTH.ADH-[L1.S].F1.

Figure OTH.ADH-[L1.S].F1: Adhesion Factor Splippery rail (soft key technology)

OTH.ADH-[L2.S.N].1When the value of the adhesion factor is slippery rail, the driver is informed about this by the Adhesion factor slippery rail symbol (ST02) as indicated in Figure OTH.ADH-[L2.S.N].F1.

Figure OTH.ADH-[L2.S.N].F1: Adhesion Factor Slippery rail (soft key technology)

OTH.ADH-[L0N1.T.N].1To modify the adhesion factor, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.ADH-[L0N1.T.N].F1.

Figure OTH.ADH-[L0N1.T.N].F1: Special button on Default window (touch screen technology)

OTH.ADH-[L2.T.N].2To modify the adhesion factor, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.ADH-[L2.T.N].F2.

Figure OTH.ADH-[L2.T.N].F2: Special button on Default window (touch screen technology)

OTH.ADH-[L0N1.S.N].1To modify the adhesion factor, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.ADH-[L0N1.S.N].F1.

Figure OTH.ADH-[L0N1.S.N].F1: Special button on Default window (soft key technology)

OTH.ADH-[L2.S.N].2To modify the adhesion factor, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.ADH-[L2.S.N].F2.

Figure OTH.ADH-[L2.S.N].F2: Special button on Default window (soft key technology)

OTH.ADH-[L0N1.T.N].2The driver shall then select the button on the Special window as indicated in Figure OTH.ADH-[L0N1.T.N].F2.

Figure OTH.ADH-[L0N1.T.N].F2: Adhesion button on the Special window (touch screen technology)

OTH.ADH-[L2.T.N].3The driver shall then select the button on the Special window as indicated in Figure OTH.ADH-[L2.T.N].F3.

Figure OTH.ADH-[L2.T.N].F3: Adhesion button on the Special window (touch screen technology)

OTH.ADH-[L0N1.S.N].2The driver shall then select the button associated to the Adhesion label on the Special window as indicated in Figure OTH.ADH-[L0N1.S.N].F2.

Figure OTH.ADH-[L0N1.S.N].F2: Adhesion button on Special window (soft key technology)

OTH.ADH-[L2.S.N].3The driver shall then select the button associated to the Adhesion label on the Special window as indicated in Figure OTH.ADH-[L2.S.N].F3.

Figure OTH.ADH-[L2.S.N].F3: Adhesion button on Special window (soft key technology)

OTH.ADH-[112021.N].2The Adhesion button is enabled when:

1. The train is at standstill AND the mode is SB AND the modification of adhesion factor by the driver is allowed by national value AND the Driver ID, train data and ETCS level are valid, OR
2. The modification of adhesion factor by the driver is allowed by national value AND the mode is FS/LS/SR/OS/UN/SN).

OTH.ADH-[22.N].2The Adhesion button is enabled when:

1. The train is at standstill AND the mode is SB AND the modification of adhesion factor by the driver is allowed by national value AND the Driver ID, train data and ETCS level are valid, OR
2. The modification of adhesion factor by the driver is allowed by national value AND the mode is FS/AD/LS/SR/OS/UN/SN).

OTH.ADH-[30.N].2The Adhesion button is enabled when:

1. The train is at standstill AND the mode is SB AND the modification of adhesion factor by the driver is allowed by national value AND the Driver ID, train data and ETCS level are valid, OR
2. The modification of adhesion factor by the driver is allowed by national value AND the mode is FS/AD/SM/LS/SR/OS/UN/SN).

OTH.ADH-[L0N1.T.N].3The driver shall enter or re-validate the adhesion status by pressing the button (1), if the adhesion is non slippery, or the button (2), if the adhesion is slippery, as indicated in Figure OTH.ADH-[L0N1.T.N].F3.

Figure OTH.ADH-[L0N1.T.N].F3: Adhesion window (soft key technology)

OTH.ADH-[L2.T.N].4The driver shall enter or re-validate the adhesion status by pressing the button (1), if the adhesion is non slippery, or the button (2), if the adhesion is slippery, as indicated in Figure OTH.ADH-[L2.T.N].F4.

Figure OTH.ADH-[L2.T.N].F4: Adhesion window (touch screen technology)

OTH.ADH-[L0N1.S.N].3The driver shall enter or re-validate the adhesion status by pressing the button with the Non slippery rail label (1), if the adhesion is non slippery, or the button with the Slippery rail label (2), if the adhesion is slippery, as indicated in Figure OTH.ADH-[L0N1.S.N].F3.

Figure OTH.ADH-[L0N1.S.N].F3: Adhesion window (touch screen technology)

OTH.ADH-[L2.S.N].4The driver shall enter or re-validate the adhesion status by pressing the button with the Non slippery rail label (1), if the adhesion is non slippery, or the button with the Slippery rail label (2), if the adhesion is slippery, as indicated in Figure OTH.ADH-[L2.S.N].F4.

Figure OTH.ADH-[L2.S.N].F4: Adhesion window (soft key technology)

OTH.ADH-[L2.S.N].4The driver shall enter or re-validate the adhesion status by pressing the button with the Non slippery rail label (1), if the adhesion is non slippery, or the button with the Slippery rail label (2), if the adhesion is slippery, as indicated in Figure OTH.ADH-[L2.S.N].F4.

Figure OTH.ADH-[L2.S.N].F4: Adhesion window (soft key technology)

## OTH.BMIInhibition of balise transmission alarm (BMI)

OTH.BMI-[30].1When the balise reading antenna is over a large metallic object that exceeds the interference limits set in the Eurobalise Form Fit Functional Interface Specification (something usually called “Big Metal Mass” and in the following referred to as “BMM”) an alarm may be generated by the balise transmission system, which in turn may trigger an on-board safe reaction.

Such “integrity check alarm of balise transmission” (in the following: “BTM alarm”) that may be generated when the balise antenna is over a BMM is not distinguishable from one that may be generated when the on-board balise reader system is in failure.

Since it is not possible for the on-board to know whether the alarm was generated by a failure (and therefore the on-board may be unable to read balises) or by the presence of a BMM under the balise antenna, it is possible that a safe reaction is taken by the on-board (for example switch to SF) when it is in fact still able to read balises.

The track condition “Big Metal Mass” provides a means for trackside to mark areas where BMMs are known to exist, and so to avoid that the on-board may take a safe reaction when there is no need to (the on-board is able to detect balises but the antenna is over a BMM).

However, there may be instances where the train is over a known BMM but the related track condition is not available on-board. For example, because the train is awakening on a metal covered area or because the driver had to select override and move the train over a metal covered area. This can result in deadlocks.

To avoid that, the procedure detailed in this section provides a means for the driver to inhibit the potential safe reaction to a BTM alarm. This in turn enables a SoM or a generic movement over a BMM in an ETCS equipped area (level 1 or 2) when no BMM track condition is stored on-board.

OTH.BMI-[30].2The driver should use the “Inhibition” procedure only when authorised to do so. This authorisation should be covered by operational procedures because to inhibit a safe reaction may be detrimental to safety.

In addition, a provision is introduced to allow the procedure to be automatically triggered without driver intervention. This provision applies in case the train is in an area covered by a BMM track condition stored on board, and the track condition gets reset (for example because of a transition to SR mode caused by Override activation).

OTH.BMI-[30.L1.T].1When the train has the BTM alarm reaction inhibition activated, the driver is informed about this by the Big Metal Mass reaction inhibition symbol (ST07) as indicated in Figure OTH.BMI-[30.L1.T].F1.

Figure OTH.BMI-[30.L1.T].F1: Big Metal Mass reaction inhibition (touch screen technology)

OTH.BMI-[30.L2.T].1When the train has the BTM alarm reaction inhibition activated, the driver is informed about this by the Big Metal Mass reaction inhibition symbol (ST07) as indicated in Figure OTH.BMI-[30.L2.T].F1.

Figure OTH.BMI-[30.L2.T].F1: Big Metal Mass reaction inhibition (touch screen technology)

OTH.BMI-[30.L1.S].1When the train has BTM alarm reaction inhibition activated, the driver is informed about this by the Big Metal Mass reaction inhibition symbol (ST07) as indicated in Figure OTH.BMI-[30.L1.S].F1.

Figure OTH.BMI-[30.L1.S].F1: Big Metal Mass reaction inhibition (soft key technology)

OTH.BMI-[30.L2.S].1When the train has the BTM alarm reaction inhibition activated, the driver is informed about this by the Big Metal Mass reaction inhibition symbol (ST07) as indicated in Figure OTH.BMI-[30.L2.S].F1.

Figure OTH.BMI-[30.L2.S].F1: Big Metal Mass reaction inhibition (soft key technology)

OTH.BMI-[30.L1.T.N].1To activate or de-activate the BTM alarm reaction inhibition, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.BMI-[30.L1.T.N].F1.

Figure OTH.BMI-[30.L1.T.N].F1: Special button on Default window (touch screen technology)

OTH.BMI-[30.L2.T.N].1To activate or de-activate the BTM alarm reaction inhibition, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.BMI-[30.L2.T.N].F1.

Figure OTH.BMI-[30.L2.T.N].F1: Special button on Default window (touch screen technology)

OTH.BMI-[30.L1.S.N].1To activate or de-activate the BTM alarm reaction inhibition, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.BMI-[30.L1.S.N].F1.

Figure OTH.BMI-[30.L1.S.N].F1: Special button on Default window (soft key technology)

OTH.BMI-[30.L2.S.N].1To activate or de-activate the BTM alarm reaction inhibition, the driver shall press the button on the Default window of the DMI as indicated in Figure OTH.BMI-[30.L2.S.N].F1.

Figure OTH.BMI-[30.L2.S.N].F1: Special button on Default window (soft key technology)

OTH.BMI-[30.L1.T.N].2To activate the BTM alarm reaction inhibition, the driver shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L1.T.N].F2.

Figure OTH.BMI-[30.L1.T.N].F2: BMM reaction inhibition on the Special window (touch screen technology)

OTH.BMI-[30.L2.T.N].2To activate the BTM alarm reaction inhibition, the driver shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L2.T.N].F2.

Figure OTH.BMI-[30.L2.T.N].F2: BMM reaction inhibition button on the Special window (touch screen technology)

OTH.BMI-[30.L1.S.N].2To activate the BTM alarm reaction inhibition, the driver shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L1.S.N].F2.

Figure OTH.BMI-[30.L1.S.N].F2: BMM reaction inhibition on the Special window (soft key technology)

OTH.BMI-[30.L2.S.N].2To activate the BTM alarm reaction inhibition, the driver shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L2.S.N].F2.

Figure OTH.BMI-[30.L2.S.N].F2: BMM reaction inhibition button on the Special window (soft key technology)

OTH.BMI-[30.L12.N].1Once the driver has elected to activate the BTM reaction inhibition, the driver is presented with the Default window.

OTH.BMI-[30.L12.N].2The BMM reaction inhibition button is enabled when:

1. The train is at standstill AND the mode is SB AND the Driver ID & train data are valid AND ETCS level is 1/2 AND “BTM alarm reaction inhibition” function is not active OR
2. The train is at standstill AND the mode is SR/SH AND ETCS level is 1/2 AND the “BTM alarm reaction inhibition” function is not active.

OTH.BMI-[30.L12.N].3The “Inhibition” procedure shall end when at least one of the following conditions is fulfilled:

1. The train has run more than the pre-defined fixed distance of 300m after the procedure was triggered, OR
2. The ERTMS/ETCS on-board equipment switches to a mode different than Standby, Shunting or Staff Responsible, OR
3. The driver ends the procedure, by revoking the inhibition.

Regarding a) above, the distance is the one travelled away from the location when the procedure was triggered and it shall be applicable in both directions.

OTH.BMI-[30.L12.N].4If a BMM track condition which announces a BMM area within the remaining distance of the manual or automatic inhibition is received, the distance for ending the procedure shall be shortened to the start of the announced BMM area.

OTH.BMI-[30.L12.N].5The driver may revoke the inhibition following an operational procedure. For example, in the case of awakening over a BMM the train has moved past the limit of the metallic covered area and so there is no longer need to have the inhibition active. Revoking the inhibition in turn increases safety, because it allows the on-board to have a safe reaction should there be a failure in the balise reader system that was until then “masked” by the inhibition set manually or automatically.

OTH.BMI-[30.L1.T.N].3To revoke the BTM alarm reaction inhibition, the driver shall access the Special window as indicated previously and shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L1.T.N].F3.

Figure OTH.BMI-[30.L1.T.N].F3: Revoke BMM reaction inhibition button on the Special window (touch screen technology)

OTH.BMI-[30.L2.T.N].3To revoke the BTM alarm reaction inhibition, the driver shall access the Special window as indicated previously and shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L2.T.N].F3.

Figure OTH.BMI-[30.L2.T.N].F3: Revoke BMM reaction inhibition button on the Special window (touch screen technology)

OTH.BMI-[30.L1.S.N].3To revoke the BTM alarm reaction inhibition, the driver shall access the Special window as indicated previously and shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L1.S.N].F3.

Figure OTH.BMI-[30.L1.S.N].F3: Revoke BMM reaction inhibition button on the Special window (soft key technology)

OTH.BMI-[30.L2.S.N].3To revoke the BTM alarm reaction inhibition, the driver shall access the Special window as indicated previously and shall then select the button on the Special window as indicated in Figure OTH.BMI-[30.L2.S.N].F3.

Figure OTH.BMI-[30.L2.S.N].F3: Revoke BMM reaction inhibition button on the Special window (soft key technology)

OTH.BMI-[30.L12.N].6Once the driver has elected to revoke the BTM reaction inhibition, the BMM reaction inhibition symbol ST07 is no longer displayed on the DMI and the driver is presented with the Default window.

OTH.BMI-[30.L12.N].7The Revoke BMM reaction inhibition button is enabled when:

1. The train is at standstill AND the mode is SB AND the Driver ID & train data are valid AND ETCS level is 1/2 AND “BTM alarm reaction inhibition” function is active OR
2. The train is at standstill AND the mode is SR/SH AND ETCS level is 1/2 AND the “BTM alarm reaction inhibition” function is active.

## OTH.ORNChange of Train Orientation (ORN)

OTH.ORN.1The driver can control the train from the front cab with the direction controller in the forward position. However, to change the orientation of the train, the driver has to change the driving cab.

Different situations can occur under these circumstances.

OTH.ORN-[V].1The driver changes of cab but uses the same engine (a mission is ongoing).

In this situation the driver closes Desk A and leaves Cab A of the leading engine of the train, to go to Cab B and open Desk B of the same engine (both desks are connected to the same ERTMS/ETCS on-board system).

When the driver closes Desk A (see section OFF.CLS Close the desk (CLS)), the mode immediately changes to Stand-By, which is considered as an end of mission.

When the driver then opens Desk B, the SB symbol is displayed (see section SB - Stand-By (SB)).

OTH.ORN-[V].2The driver changes cab and leaves one engine to go to another engine.

In this situation the train has two engines available (Engine A and Engine B). Engine A is the leading engine and Engine B is the slave engine. Each engine has its own ETCS on-board equipment.

1. Case A: Engine B is in SL mode.

   The driver closes Desk A of Engine A (see section OFF.CLS Close the desk (CLS)), any mission in progress is finished and the mode changes to Stand-By mode.

   The ETCS on-board equipment of Engine B switches to Stand-By mode.

   The driver leaves Engine A and enters Engine B. When the driver opens Desk B in Engine B a new mission is triggered (see section SB - Stand-By (SB)).

2. Case B: Engine B is in NL mode.

   The driver selects Non-Leading on Desk A of Engine A (see section NL - Non-Leading (NL)), the ETCS on-board equipment changes to Non-Leading mode.

   Once the Non-Leading signal is not received, Engine B mode changes to Stand-By mode (see section SB - Stand-By (SB)).

3. Case C: Engine B is in PS mode.

   The driver selects Maintain Shunting on Desk A of Engine A (see section SH.PS Maintain SH when changing the cab (PS)), the mode changes to Passive Shunting mode once the driver closes Desk A of Engine A.

   If the driver opens Desk B of Engine B, the ETCS on-board equipment switches Desk B to Shunting mode (see section SH - Shunting (SH)).

OTH.ORN-[V].3The driver changes cab but uses the same engine, while a Shunting movement is ongoing.

In this situation the driver closes Desk A and leaves Cab A. The driver then goes to Cab B and opens Desk B of this same engine while the ETCS on-board equipment is in Shunting mode.

Both Desk A and Desk B are connected to the same ETCS on-board system.

When the driver closes Desk A of Cab A, if the driver has previously selected the function Maintain Shunting (see section SH.PS Maintain SH when changing the cab (PS)), the mode immediately changes to Passive Shunting mode.

When the driver opens Desk B of Cab B, the ETCS on-board equipment switches back to Shunting mode (see section SH - Shunting (SH)).

## OTH.JOIJoining (JOI)

OTH.JOI.1When the Joining procedure happens:

1. The joining train (train performing the Joining operation) approaches the train to be joined. This can be performed in SR, OS or SH mode.
2. The electrical and mechanical links between the two trains are closed.

OTH.JOI-[30].1The procedure can also be performed in SM mode.

OTH.JOI-[V].1Train specific clauses indicating how to close the electrical and mechanical links.

OTH.JOI.2If a mission is still in progress after the joining procedure, the driver must modify the Train Data such that it fits with the new train composition (see section OTH.DAT.MAN Manual change of train data (MAN)).

OTH.JOI.3If a former leading ETCS on-board equipment is to become slave equipment in NL mode, the driver shall select NL mode (see section NL - Non-Leading (NL)).

OTH.JOI-[V].2Information that a Joining operation has been correctly completed is not provided for the ETCS equipment. Joining operation requires the fulfilment of operating rules ensuring that a Joining operation has been correctly completed (e.g. physical connection).

OTH.JOI.4In a case when a train has to enter an occupied track section, as is the case for a joining operation, the signaller shall, before authorising the entry to the occupied track section, obtain confirmation that the occupying train or vehicles will not move towards the train entering the occupied track section.

## OTH.SPLSplitting (SPL)

OTH.SPL.1When the Splitting procedure happens:

1. The electrical and mechanical links between the two trains are removed.
2. If Splitting procedure requires moving the two train parts apart from each other for a small distance, this can be done even in SB mode.

The Splitting procedure must be performed while the train is at standstill.

The Splitting procedure can only be performed if the two resulting trains both have, at least, one ETCS on-board equipment each.

OTH.SPL-[V].1Train specific clauses indicating how to remove the electrical and mechanical links between the two train.

OTH.SPL.2If the ETCS on-board equipment which was supervising the train before splitting has not performed an End of Mission for splitting. The driver must modify the Train Data such that it fits with the new train composition (see section OTH.DAT.MAN Manual change of train data (MAN)).

OTH.SPL.3The driver can then start a new mission, Shunting movements or not move the train depending on the case.

OTH.SPL-[V].2Information that a Splitting operation has been correctly completed is not provide for the ETCS on-board equipment. Splitting operation requires the fulfilment of operating rules ensuring that a Splitting operation has been correctly completed (e.g. physical disconnection).

## OTH.TXTText message from trackside (TXT)

OTH.TXT-[L0N1.T].1The driver can receive information from the trackside in the form of text messages displayed on the DMI screen as indicated in Figure OTH.TXT-[L0N1.T].F1.

Figure OTH.TXT-[L0N1.T].F1: Text message (touch screen technology)

OTH.TXT-[L2.T].1The driver can receive information from the trackside in the form of text messages displayed on the DMI screen as indicated in Figure OTH.TXT-[L2.T].F1.

Figure OTH.TXT-[L2.T].F1: Text message (touch screen technology)

OTH.TXT-[L0N1.S].1The driver can receive information from the trackside in the form of text messages displayed on the DMI screen as indicated in Figure OTH.TXT-[L0N1.S].F1.

Figure OTH.TXT-[L0N1.S].F1: Text message (soft key technology)

OTH.TXT-[L2.S].1The driver can receive information from the trackside in the form of text messages displayed on the DMI screen as indicated in Figure OTH.TXT-[L2.S].F1.

Figure OTH.TXT-[L2.S].F1: Text message (soft key technology)

OTH.TXT-[L0N1.T].2When there is more than one text message displayed, the driver can scroll through the list of text messages by pressing the and buttons as indicated in Figure OTH.TXT-[L0N1.T].F2.

Figure OTH.TXT-[L0N1.T].F2:[Up] and [Down] buttons (touch screen technology)

OTH.TXT-[L2.T].2When there is more than one text message displayed, the driver can scroll through the list of text messages by pressing the and buttons as indicated in Figure OTH.TXT-[L2.T].F2.

Figure OTH.TXT-[L2.T].F2:[Up] and [Down] buttons (touch screen technology)

OTH.TXT-[L0N1.S].2When there is more than one text message displayed, the driver can scroll through the list of text messages by pressing the and buttons as indicated in Figure OTH.TXT-[L0N1.S].F2.

Figure OTH.TXT-[L0N1.S].F2:[Up] and [Down] buttons (soft key technology )

OTH.TXT-[L2.S].2When there is more than one text message displayed, the driver can scroll through the list of text messages by pressing the and buttons as indicated in Figure OTH.TXT-[L2.S].F2.

Figure OTH.TXT-[L2.S].F2:[Up] and [Down] buttons (soft key technology)

OTH.TXT.1There are some text messages that require driver acknowledgement. They are displayed with a flashing frame and when they appear for the first time the Sinfo sound is played.

OTH.TXT-[L0N1.T].3To acknowledge this kind of text message, the driver shall press on the text message itself as indicated in Figure OTH.TXT-[L0N1.T].F3.

Figure OTH.TXT-[L0N1.T].F3: Text message acknowledgement (touch screen technology)

OTH.TXT-[L2.T].3To acknowledge this kind of text message, the driver shall press on the text message itself as indicated in Figure OTH.TXT-[L2.T].F3.

Figure OTH.TXT-[L2.T].F3: Text message acknowledgement (touch screen technology)

OTH.TXT-[L0N1.S].3To acknowledge this kind of text message, the driver shall press the button associated to the text message as indicated in Figure OTH.TXT-[L0N1.S].F3.

Figure OTH.TXT-[L0N1.S].F3: Text message acknowledgement (soft key technology)

OTH.TXT-[L2.S].3To acknowledge this kind of text messages, the driver shall press the button associated to the text message as indicated in Figure OTH.TXT-[L2.S].F3.

Figure OTH.TXT-[L2.S].F3:Text message acknowledgement (soft key technology)

OTH.TXT.2Text messages remain displayed until they are acknowledged by the driver.

In some cases, the brake is applied if the driver does not acknowledge the text message before the end condition is reached.

OTH.TXT-[11].1If the driver acknowledges the text message before the end condition is fulfilled, the text message disappears from the DMI.

OTH.TXT-[20212230].1If the driver acknowledges the text message before the end condition is fulfilled, the text display can end or not depending on the end condition.

## OTH.BRKBrake command handling (BRK)

OTH.BRK.1The driver is informed that the brake command has been triggered when the Service Brake or Emergency Brake Intervention following symbol (ST01) is displayed:

ST01: Service brake or emergency brake intervention

In addition, when the brake is not applied due to an overspeed of the permitted speed, a text message is displayed indicating the reason that caused the brake command to be triggered. Depending on the reason for the activation of the brake command, the brake release occurs under some conditions or other.

1. When the emergency brake command is triggered due to a trip transition, a text message with the Trip condition is displayed (see section DEG.TR Transition to Trip mode (TR)). In this case, the emergency brake command is released at standstill and after the driver acknowledgment of the trip condition.
2. The “Balise read error” text message is displayed when the brake command is triggered due to linking error, balise group message inconsistency or RAMS related supervision error. In this case the brake command is released at standstill (see section DEG.BLS Managing a balise read error (BLS)).
3. The “Communication error” text message is displayed when the brake command is triggered due to supervision of the safe radio connection. In this case the brake command is released at standstill or when a new consistent message has been received from the RBC (see section DEG.RBC Managing absence of RBC information (RBC)).
4. The “Runaway movement” text message is displayed when the brake command is triggered due to the detection of a train movement exceeding the allowed roll away distance, the allowed reverse distance, the standstill supervision distance or distance allowed for reverse movement in Post Trip mode, or while the driver is modifying the Train data or is entering the SR speed/ distance limits. In this case, the brake command is released at standstill and after driver acknowledgement (see section OTH.BRK.UNI Reacting to unintentional movements (UNI)).
5. The “Train data changed” text message is displayed when the brake command is triggered due to change of Train Data while the train is running. In this case, the brake command is released at standstill and after driver acknowledgement (see section OTH.DAT.EXT Change of train data by ETCS external sources (EXT)).
6. The “RV distance exceeded” text message is displayed when the brake command is triggered due to an overpassed reversing distance related to a reversing area. In this case, the brake command shall be released if the reversing distance becomes extended so that the reversing distance is no longer overpassed, or at standstill after driver acknowledgement (see section RV.RUN Running in RV (RUN)).

When the brake command is triggered due to the driver not having acknowledged a text message, the brake command is released only after the driver acknowledges the text message (see section OTH.TXT Text message from trackside (TXT)).

OTH.BRK-[B41].1The “PT distance exceeded” text message is displayed when the brake command is triggered due to the detection of a train movement exceeding the distance allowed for reverse movement in Post Trip mode. In this case, the brake command shall be released at standstill.

OTH.BRK-[30].1The “Safe consist length no longer available” text message is displayed when the brake command is triggered due the safe consist length information acquired from an external source becoming unavailable. In this case, the brake command shall be released at standstill.

OTH.BRK.2If the driver’s acknowledgement is not needed to release the brake, the driver is warned that the brake has been released with the Sinfo sound.

OTH.BRK.3Otherwise, when driver’s acknowledgement is necessary to release the brake command, the Sinfo sound is played to draw the driver’s attention to this acknowledgement.

OTH.BRK.4In case more than one reason to command the brake is applicable at the same time, the brake command shall be released only when the release conditions specified including the concerned reasons have been fulfilled. In particular, if several brake command reasons applicable at the same time are included in several clauses where a driver acknowledgement is required, there shall be as many individual driver acknowledgements required as concerned reasons.

OTH.BRK.5In case of an ETCS mode change, the ERTMS/ETCS on-board equipment shall maintain the brake command if at least one individual brake command reason remains applicable, until the corresponding release conditions have been all fulfilled.

Upon a mode change, the ERTMS/ETCS on-board equipment shall maintain the brake command if at least one individual brake command reason remains applicable, until the corresponding release conditions have been all fulfilled.

OTH.BRK.6The service brake command (SBC) is defined as a two state output with the following values:

1. Service brake commanded
2. Service brake not commanded.

The SBC output is generated by ERTMS/ETCS on-board to command the service brake and to revoke this command.

The SBC output value Service brake commanded shall result in the train applying the full service brake, meaning application of 100% of the installed braking performance of the train, and cutting off the traction.

OTH.BRK.7The SBC output value Service brake not commanded shall result in a release of the service brake, but only to the highest brake level currently commanded by other application(s) or by the driver, and shall permit the traction power to be switched on.

The traction power can be switched on again only after the driver has cancelled the traction command (i.e. after a 0-position-acknowledgement by the traction controller).

OTH.BRK.8In case of no SB manually applied by the driver and in case of no Automatic Speed Control activated, the SB released by ETCS will automatically cancel the brake application on the train. In case of a gradient, it is possible to have forward movement which must be controlled by driver with his own action on brake. This is acceptable as it is the same situation today (without ETCS).

OTH.BRK.9The full service brake may be actuated by various brake systems depending on the rolling stock brake architecture (e.g. dynamic brake by substitution, blending or superposition principle with the UIC air brake).

OTH.BRK.10A brake application command, whatever its control mode, takes control of the brake system, even in case of active brake release command; this may not to apply when intentional suppression of the brake application command is given by the driver (e.g. passenger alarm override, uncoupling).

OTH.BRK-[L0N1.T].1To acknowledge a brake intervention and to release the brake the driver shall press the button which has a flashing frame as indicated in Figure BRK-[L0N1.T].F1.

Figure BRK-[L0N1.T].F1: Brake intervention to be acknowledged (touch screen technology)

OTH.BRK-[L2.T].1To acknowledge a brake intervention and to release the brake the driver shall press the button which has a flashing frame as indicated in Figure BRK-[L2.T].F1.

Figure BRK-[L2.T].F1: Brake intervention to be acknowledged (touch screen technology)

OTH.BRK-[L0N1.S].1To acknowledge a brake intervention and to release the brake the driver shall press the button associated to the Brake command symbol (ST01) as indicated in Figure BRK-[L0N1.S].F1.

Figure BRK-[L0N1.S].F1: Brake intervention to be acknowledged (soft key technology)

OTH.BRK-[L2.S].1To acknowledge a brake intervention and to release the brake the driver shall press the button associated to the Brake command symbol (ST01) as indicated in Figure BRK-[L2.S].F1.

Figure BRK-[L2.S].F1: Brake intervention to be acknowledged (soft key technology)

### OTH.BRK.UNIReacting to unintentional movements (UNI)

OTH.BRK.UNI-[L12.N].1If after being at a standstill, the train movement or Shunting movement has moved unintentionally and exceeded the allowed distance defined by a National Value, the ETCS on-board triggers the brake and the “Runaway movement” text message is displayed.

In this situation, the driver shall secure the train or Shunting movement according to non-harmonised rules and acknowledge the brake application.

### OTH.BRK.DIRDirect brake (DIR)

OTH.BRK.DIR.1Locomotives assessed for general operation shall be fitted with a direct brake system which allows the application of a brake force on the concerned unit(s) independently of the main brake command, with other unit(s) of the train remaining without brake applied.

### OTH.BRK.DYNDynamic braking (DYN)

OTH.BRK.DYN.1If a unit is equipped with a dynamic brake system, it is possible to prevent the use of regenerative braking on electric units so that there is no return of energy to the overhead contact line when driving on a line which does not allow that.

OTH.BRK.DYN.2The subsequent commands of regenerative brake inhibition by the unit can be automatic or manual through intervention of the driver.

OTH.BRK.DYN.3Dynamic brake can be used independently from other brake systems, or together with other brake systems (blending).

OTH.BRK.DYN.4Where on locomotives the dynamic brake is used independently from other brake systems, the maximum value and rate of variation of the dynamic brake effort can be limited to predefined values.

### OTH.BRK.EDYEddy current track brake (EDY)

OTH.BRK.EDY.1The conditions for use of eddy current track brake for technical compatibility with the track are not harmonised. The commands of inhibition of eddy current track brake by the unit can be automatic or manual through intervention of the driver.

### OTH.BRK.EMGEmergency brake (EMG)

OTH.BRK.EMG.1At least two independent emergency brake command devices are available to the driver, allowing the activation of the emergency brake by a simple and single action from the driver in his normal driving position, using one hand.

OTH.BRK.EMG.2One of these devices is a red punch button (mushroom push button).

The emergency brake position of these two devices when activated is self-locking by a mechanical device; unlocking this position is then possible only by an intentional action by the staff.

### OTH.BRK.INDBrake state and fault indication (IND)

OTH.BRK.IND.1The status of the brake system must be available to the driver. The driver must be able to, at standstill and running, identify the status (applied or released or isolated) of the main (emergency and service) and parking brake systems, and the status of each part (including one or several actuators) of these systems that can be controlled and/or isolated independently.

OTH.BRK.IND.2When running, the driver shall be able to check from the driving position in the cab:

1. The status of the train brake control command line,
2. The status of the train brake energy supply,
3. The status of the dynamic brake and braking system linked to traction system where they are included in the performance of the emergency braking in normal mode,
4. The status applied or released of at least one part (actuator) of the main brake system which is controlled independently (e.g. a part which is installed on the vehicle fitted with an active cab).

### OTH.BRK.MAGMagnetic track brake (MAG)

OTH.BRK.MAG.1A magnetic track brake is allowed to be used as an emergency brake.

Magnetic track brake cannot be used at speeds higher than 280 km/h.

The commands of inhibition of magnetic track brake by the unit can be automatic or manual through intervention of the driver.

### OTH.BRK.PRKParking brake (PRK)

OTH.BRK.PRK.1Trains shall be equipped with a parking brake function used when the train is parked, allowing the application of a brake force without any available energy on board for an unlimited period of time.

OTH.BRK.PRK.2The main brake function of a train shall be:

- continuous: the brake application signal is transmitted from a central command to the whole train by a control line.
- automatic: an inadvertent disruption (loss of integrity, line de-energised, etc.) of the control line leads to brake activation on all vehicles of the train.

OTH.BRK.PRK.3The brake system shall include means for monitoring and tests available to the driver.

OTH.BRK.PRK.4The parking braking command leads to the application of a defined brake force for an unlimited period of time, during which a lack of any energy on board may occur.

OTH.BRK.PRK.5The parking brake can be released at standstill, including for rescue purposes.

OTH.BRK.PRK.6For units assessed in fixed or predefined formations, and for locomotives assessed for general operation, the parking brake command must be activated automatically when the unit is switched off. For other units, the parking brake command is either activated manually, or activated automatically when the unit is switched off.

OTH.BRK.PRK.7The application of the parking brake force may depend on the status of the main brake function; it is effective when the energy on board to apply the main brake function is lost or is going to increase or decrease (after having switched on or off the unit).

### OTH.BRK.SVCService brake (SVC)

OTH.BRK.SVC.1The service brake function allows the driver to adjust (by application or release) the brake force between a minimum and a maximum value in a range of at least 7 steps (including brake release and maximum brake force), in order to control the speed of the train.

OTH.BRK.SVC.2The service braking command is active only in one location in a train. This means that it is possible to isolate the service braking function of the other service braking command(s) of the unit(s) part of a train formation, as defined for fixed and predefined formations.

OTH.BRK.SVC.3When the speed of the train is higher than 15 km/h, the service brake activation by the driver leads automatically to the cut-off of all tractive effort; this cut-off is not reset until the traction command is cancelled by the driver.

OTH.BRK.SVC.4In case of service brake and traction controlled by automatic speed regulation, the traction cut-off is not required to be cancelled by the driver.

## OTH.INTDriver confirmation of train integrity (INT)

OTH.INT.1The Train integrity information is given either by an external device or by the driver.

When requested by the signaller to manually confirm train integrity on the DMI, the driver shall do so only at standstill and according to RU rules.

OTH.INT-[N].1Network specific clauses explaining the non-harmonised rules to confirm the Train integrity by the driver.

OTH.INT-[L0N1.T].1To confirm the Train integrity, the driver shall first get access to the Special window by pressing the button on the Default window of the DMI as indicated in Figure OTH.INT-[L0N1.T].F1.

Figure OTH.INT-[L0N1.T].F1: Special button on Default window (touch screen technology)

OTH.INT-[L2.T].1To confirm the Train integrity, the driver shall first get access to the Special window by pressing the button on the Default window of the DMI as indicated in Figure OTH.INT-[L2.T].F1.

Figure OTH.INT-[L2.T].F1: Special button on Default window (touch screen technology)

OTH.INT-[L0N1.S].1To confirm the Train integrity, the driver shall first get access to the Special window by pressing the button on the Default window of the DMI as indicated in Figure OTH.INT-[L0N1.S].F1.

Figure OTH.INT-[L0N1.S].F1: Special button on Default window (soft key technology)

OTH.INT-[L2.S].1To confirm the Train integrity, the driver shall first get access to the Special window by pressing the button on the Default window of the DMI as indicated in Figure OTH.INT-[L2.S].F1.

Figure OTH.INT-[L2.S].F1: Special button on Default window (soft key technology)

OTH.INT-[L0N1.T].2The driver shall then confirm the Train integrity by selecting the button in the Special window as indicated in Figure OTH.INT-[L0N1.T].F2.

Figure OTH.INT-[L0N1.T].F2: Train integrity button on the Special window (touch screen technology)

OTH.INT-[L2.T].2The driver shall then confirm the Train integrity by selecting the button in the Special window as indicated in Figure OTH.INT-[L2.T].F2.

Figure OTH.INT-[L2.T].F2: Train integrity button on the Special window (touch screen technology)

OTH.INT-[L0N1.S].2The driver shall then confirm the Train integrity by selecting the button associated to the Train integrity label in the Special window as indicated in Figure OTH.INT-[L0N1.S].F2.

Figure OTH.INT-[L0N1.S].F2: Train integrity button on Special window (soft key technology)

OTH.INT-[L2.S].2The driver shall then confirm the Train integrity by selecting the button associated to the Train integrity label in the Special window as indicated in Figure OTH.INT-[L2.S].F2.

Figure OTH.INT-[L2.S].F2: Train integrity button on Special window (soft key technology)

OTH.INT.2The button is a delay-type button, meaning that the driver must keep pressing during 2 seconds to be considered by the DMI. If the button is pressed by the driver for less than the 2 seconds, no valid request to confirm train integrity shall be considered by the onboard.

OTH.INT-[112021].1The button is enabled when:

1. The train is at standstill AND,
2. The mode is SB/FS/LS/SR/OS/PT AND,
3. The Driver ID, train data AND ERTMS/ETCS level are valid.

OTH.INT-[22].1The button is enabled when:

1. The train is at standstill AND,
2. The mode is SB/FS/AD/LS/SR/OS/PT AND,
3. The Driver ID, train data AND ERTMS/ETCS level are valid.

OTH.INT-[30].1The button is enabled when:

1. The train is at standstill AND,
2. The mode is SB/FS/AD/AD/LS/SR/OS/PT AND,
3. The Driver ID, train data AND ERTMS/ETCS level are valid.

## OTH.GEOGeographical position reporting (GEO)

OTH.GEO-[T].1The driver has the possibility to check the Geographical position of the train in relation to the track kilometre from the DMI if this information is available on the ETCS on-board equipment.

When the Geographical position is available but the Geographical position function is toggled off the Geographical Position symbol (DR03, located in area G12) is displayed on the DMI:

DR03: Geographical Position

When the Geographical position is toggled on, the symbol DR03 is replaced by the numerical value of the position.

OTH.GEO-[S].1The driver has the possibility to check the Geographical position of the train in relation to the track kilometre from the DMI if this information is available on the ETCS on-board equipment.

When the Geographical position is available but the Geographical position function is toggled off the Geographical Position symbol (DR03, located in area F8) is displayed on the DMI:

DR03: Geographical Position

When the Geographical position is toggled on, the numerical value of the position is displayed above the symbol DR03.

OTH.GEO-[L0N1.T].1To toggle on the display of the Geographical position, the driver shall press the button with the symbol DR03. To toggle off the display of the Geographical position, the driver shall press the button with the numerical position value returning to the initial state as indicated in Figure OTH.GEO-[L0N1.T].F1.

Figure OTH.GEO-[L0N1.T].F1: Geographical Position (touch screen technology)

OTH.GEO-[L2.T].1To toggle on the display of the Geographical position, the driver shall press the button with the symbol DR03. To toggle off the display of the Geographical position, the driver shall press the button with the numerical position value returning to the initial state as indicated in Figure OTH.GEO-[L2.T].F1.

Figure OTH.GEO-[L2.T].F1: Geographical Position (touch screen technology)

OTH.GEO-[L0N1.S].1To toggle on or off the display of the Geographical position, the driver shall press the button (DR03) as indicated in Figure OTH.GEO-[L0N1.S].F1.

Figure OTH.GEO-[L0N1.S].F1: Geographical Position (soft key technology)

OTH.GEO-[L2.S].1To toggle on or off the display of the Geographical position, the driver shall press the button (DR03) as indicated in Figure OTH.GEO-[L2.S].F1.

Figure OTH.GEO-[L2.S].F1: Geographical Position (soft key technology)

## OTH.ATOAutomatic Train Operation selector (ATO)

OTH.ATO-[2230.V].1The driver has the possibility, through an ATO selector, to enable/disable the automatic driving and the display of the information related to the ERTMS/ATO subsystem, with the exception of the ATO data entry/view. The ATO selector position ("On" or "Stand-by") applicable when the ERTMS/ETCS on-board equipment is switched off (i.e. enters No Power mode) shall be retained and shall remain applicable when powered on.

OTH.ATO-[2230.L1.T.V].1To access the ATO selector, the driver shall first get access to the Settings window by pressing the button on the Default window of the DMI as indicated in Figure OTH.ATO-[2230.L1.T.V].F1.

Figure OTH.ATO-[2230.L1.T.V].F1: Special button on Default window (touch screen technology)

OTH.ATO-[2230.L2.T.V].1To access the ATO selector, the driver shall first get access to the Settings window by pressing the button on the Default window of the DMI as indicated in Figure OTH.ATO-[2230.L2.T.V].F1.

Figure OTH.ATO-[2230.L2.T.V].F1: Special button on Default window (touch screen technology)

OTH.ATO-[2230.L1.S.V].1To access the ATO selector, the driver shall first get access to the Settings window by pressing the button on the Default window of the DMI as indicated in Figure OTH.ATO-[2230.L1.S.V].F1.

Figure OTH.ATO-[2230.L1.S.V].F1: Settings button on Default window (soft key technology)

OTH.ATO-[2230.L2.S.V].1To access the ATO selector, the driver shall first get access to the Settings window by pressing the button on the Default window of the DMI as indicated in Figure OTH.ATO-[2230.L2.S.V].F1.

Figure OTH.ATO-[2230.L2.S.V].F1: Settings button on Default window (soft key technology)

OTH.ATO-[2230.L1.T.V].2The driver shall then access the ATO selector by selecting the ATO button in the Settings window as indicated in Figure OTH.ATO-[2230.L1.T.V].F2.

Figure OTH.ATO-[2230.L1.T.V].F2: ATO button on the Settings window (touch screen technology)

OTH.ATO-[2230.L2.T.V].2The driver shall then access the ATO selector by selecting the ATO button in the Settings window as indicated in Figure OTH.ATO-[2230.L2.T.V].F2.

Figure OTH.ATO-[2230.L2.T.V].F2: ATO button on the Settings window (touch screen technology)

OTH.ATO-[2230.L1.S.V].2The driver shall then access the ATO selector by selecting the button associated to the ATO label in the Settings window as indicated in Figure OTH.ATO-[2230.L1.S.V].F2.

Figure OTH.ATO-[2230.L1.S.V].F2: ATO button on Special window (soft key technology)

OTH.ATO-[2230.L2.S.V].2The driver shall then access the ATO selector by selecting the button associated to the ATO label in the Settings window as indicated in Figure OTH.ATO-[2230.L2.S.V].F2.

Figure OTH.ATO-[2230.L2.S.V].F2: ATO button on Special window (soft key technology)

OTH.ATO-[22.V].1As a result, the ATO window is presented to the driver. The ATO button is enabled when:

1. The train is at standstill AND
2. The mode is SH/FS/AD/LS/SR/OS/NL/UN/TR/PT/SN/RV

OTH.ATO-[30.V].1As a result, the ATO window is presented to the driver. The ATO button is enabled when:

1. The train is at standstill AND
2. The mode is SH/FS/AD/SM/LS/SR/OS/NL/UN/TR/PT/SN/RV

OTH.ATO-[2230.L1.T.V].3The driver may then revalidate or re-enter the ATO selector position by pressing the Stand-by button or the On button (1) and confirm by pressing the input field itself (2) as indicated in Figure OTH.ATO-[2230.L1.T.V].F3.

Figure OTH.ATO-[2230.L1.T.V].F3: ATO Selector window (touch screen technology)

OTH.ATO-[2230.L2.T.V].3The driver may then revalidate or re-enter the ATO selector position by pressing the Stand-by button or the On button (1) and confirm by pressing the input field itself (2) as indicated in Figure OTH.ATO-[2230.L2.T.V].F3.

Figure OTH.ATO-[2230.L2.T.V].F3: ATO Selector window (touch screen technology)

OTH.ATO-[2230.L1.S.V].3The driver may then revalidate or re-enter the ATO selector position by pressing the button associated with the label “Stand-by” or “On” (1) and confirm by pressing the button (2) as indicated in Figure OTH.ATO-[2230.L1.S.V].F3.

Figure OTH.ATO-[2230.L1.S.V].F3: ATO Selector window (soft key technology)

OTH.ATO-[2230.L2.S.V].3The driver may then revalidate or re-enter the ATO selector position by pressing the button associated with the label “Stand-by” or “On” (1) and confirm by pressing the as indicated in Figure OTH.ATO-[2230.L2.S.V].F3. /

Figure OTH.ATO-[2230.L2.S.V].F3: ATO Selector window (soft key technology)

OTH.ATO-[2230.V].2Once the ATO selector position is re-entered or revalidated, the driver is presented with the Default window.

OTH.ATO-[2230.V].3In addition to the ATO selector window, the DMI may offer the possibility to enable/disable the automatic driving and the display of the information related to the ERTMS/ATO subsystem via other means, for example with a button positioned on an ergonomic location on the driver’s desk.