# Level Crossing (LX)

LX-[2021.L123].1When the train is approaching a Level Crossing (LX) the driver is informed if the level crossing is not protected.

LX-[2021.L123].2In FS, LS or OS modes, when the LX not protected symbol (LX01) is displayed, the driver shall apply the Rule 7 of the Appendix B in the TSI OPE.

LX01: LX not protected

LX-[2021.L1.T].1The Figure LX-[2021.L1.T].F1 shows an example of a DMI screen when the LX not protected symbol (LX01) is displayed.

Figure LX-[2021.L1.T].F1: LX not protected symbol (touch screen technology)

LX-[2021.L23.T].1The Figure LX-[2021.L23.T].F1 shows an example of a DMI screen when the LX not protected symbol (LX01) is displayed.

Figure LX-[2021.L23.T].F1: LX non protected symbol (touch screen technology)

LX-[2021.L1.S].1The Figure LX-[2021.L1.S].F1 shows an example of a DMI screen when the LX not protected symbol (LX01) is displayed.

Figure LX-[2021.L1.S].F1: LX not protected symbol (soft key technology)

LX-[2021.L23.S].1The Figure LX-[2021.L23.S].F1 shows an example of a DMI screen when the LX not protected symbol (LX01) is displayed.

Figure LX-[2021.L23.S].F1: LX not protected symbol (soft key technology)

LX-[2021.L123].3 The LX not protected symbol (LX01) is displayed until one of the following conditions is satisfied:

1. The level crossing status changes to LX protected.
2. The train passes the level crossing location.

LX-[2021.L123.N].1In SR mode, when the text message “Level crossing not protected” is displayed on the DMI, the driver shall apply Rule 7 of the Appendix B in the TSI OPE.

LX-[2021.L1.T].2The Figure LX-[2021.L1.T].F2 shows an example of a DMI screen when the text message “Level crossing not protected” in is displayed in SR mode.

Figure LX-[2021.L1.T].F2: Text message “Level crossing not protected” in SR mode (touch screen technology)

LX-[2021.L23.T].2 The Figure LX-[2021.L23.T].F2 shows an example of a DMI screen when the text message “Level crossing not protected” in is displayed in SR mode.

Figure LX-[2021.L23.T].F2: Text message “Level crossing not protected” in SR mode (touch screen technology)

LX-[2021.L1.S].2The Figure LX-[2021.L1.S].F2 shows an example of a DMI screen when the text message “Level crossing not protected” in is displayed in SR mode.

Figure LX-[2021.L1.S].F2: Text message “Level crossing not protected” in SR mode (soft key technology)

LX-[2021.L23.S].2The Figure LX-[2021.L23.S].F2 shows an example of a DMI screen when the text message “Level crossing not protected” in is displayed in SR mode.

Figure LX-[2021.L23.S].F2: Text message “Level crossing not protected” in SR mode (soft key technology)