|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *TEST CASE DESCRIPTION* | | | | | | | |
|  | | Code | Version | | | Title | |
| Test Case | | 2.17.14 | 1 | | | Level transition from LSTM ASFA to L2. Signal at proceed aspect. | |
|
| Baseline applicable | | Baseline 2 (2.3.0.d) | | | | | |
| Test case author | | ADIF | | | | | |
| Test Objective(s) | | Verify that the transition from level STM ASFA to level 2 is performed correctly. | | | | | |
| Diagram | |  | | | | | |
| Starting conditions | | Level | | | STM ASFA | | |
| Mode | | | SN | | |
| Train Speed (km/h) | | | Maximum permitted speed in STM ASFA | | |
| Additional starting conditions | | | The train is approaching the level transition to Level 2 at the maximum speed of the line and the signal at the transition border displays proceed aspect. | | |
| Sequence of the Test Case | | Checkpoints | | | | | |
| Step | Step description | Interfaces | | Description of what to be tested at the interface | | | OK? |
| 1 | The EVC receives the order to connect with the RBC via balise group. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Packet 42  NID\_RBC  NID\_RADIO  Q\_RBC = 1 | | |  |
| 2 | The EVC starts to establish safe radio connection and sends the train data to the RBC. | DMI (O) | | Safe radio connection symbol is displayed. | | |  |
| DMI (I) | |  | | |  |
| JRU | | Message 155  Message 32  Message 159  Message 129  Message 8 | | |  |
| 3 | The train receives the level transition announcement via balise group or RBC. | DMI (O) | | Level 2 transition announcement | | |  |
| DMI (I) | |  | | |  |
| JRU | | (LRBG1)  (if received from RBC Message 3/24/33)  Packet 41  D\_LEVELTR = D1  M\_LEVELTR = 3  L\_ACKLEVELTR = L1  START DISPLAYING TEXT MESSAGE (1) | | |  |
| 4 | The EVC runs the distance “D1-L1” at which the acknowledgement window of the transition to Level 2 is shown to the driver. | DMI (O) | | Level 2 Acknowledgement is displayed | | |  |
| DMI (I) | |  | | |  |
| JRU | | START DISPLAYING TEXT MESSAGE (2)  Estimated front end=D1-L1-L\_DOUBTUNDER | | |  |
| 5 | The driver acknowledges the level transition | DMI (O) | | Level 2 Acknowledgement disappears | | |  |
| DMI (I) | | Driver acknowledges the level transition. | | |  |
| JRU | | M\_DRIVERACTIONS = 8  STOP DISPLAYING TEXT MESSAGE (2) | | |  |
| 6 | The EVC receives a MA from the RBC | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Message 3  Packet 15  Packet 21  Packet 27 | | |  |
| 7 | The EVC runs the distance "D1" or the balise group with level transition order to L2 is read. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Packet 41  D\_LEVELTR = 32767  M\_LEVELTR = 3 | | |  |
| 8 | Transition to L2 is performed. | DMI (O) | | Level 2 Symbol  FS Symbol  Vpermitted does not decrease  Level 2 transition announcement disappears | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL= 3  M\_MODE = 0  STOP DISPLAYING TEXT MESSAGE (1) | | |  |
| 9 | The EVC reports to the RBC the train position due to the level transition. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Message 136  Packet 0  M\_LEVEL = 3  M\_MODE = 0 | | |  |
| Final state | | Level | | 2 | | |  |
| Mode | | FS | | |  |
| Train Speed (km/h) | | NR | | |  |
| Other parameters | |  | | |  |
| Final Test Result | |  | | | | | |
| Field of Application | | Spain | | | | | |
| Briefing instructions | |  | | | | | |