|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *TEST CASE DESCRIPTION* | | | | | | | |
|  | | Code | Version | | | Title | |
| Test Case | | 3.17.48 | 1 | | | Level transition from L2 to LSTM ASFA. TSR in LSTM area. | |
|
| Baseline applicable | | Baseline 2 (2.3.0.d) | | | | | |
| Test case author | | ADIF | | | | | |
| Test Objective(s) | | Verify that the system correctly supervises the permitted speed in the vicinity of a level transition from level 2 to LSTM ASFA when the train approaches the LSTM area and a TSR is set in the LSTM area. | | | | | |
| Diagram | |  | | | | | |
| Starting conditions | | Level | | | 2 | | |
| Mode | | | FS | | |
| Train Speed (km/h) | | | NR | | |
| Additional starting conditions | | | A TSR (or more) is set in the LSTM area close to the transition border.  A level 2 MA beyond the level transition border is stored on board. All the signals are in proceed aspect | | |
| Sequence of the Test Case | | Checkpoints | | | | | |
| Step | Step description | Interfaces | | Description of what to be tested at the interface | | | OK? |
| 1 | The train receives the level transition announcement via balise group or RBC. | DMI (O) | | Level STM ASFA transition announcement | | |  |
| DMI (I) | |  | | |  |
| JRU | | (LRBG1)  (If received from RBC Message 3/24/33)  Packet 41  D\_LEVELTR = d  M\_LEVELTR = 1  L\_ACKLEVELTR = L  NID\_STM = 0 (ASFA)  START DISPLAYING TEXT MESSAGE (1) | | |  |
| 2 | TSR information is received via RBC. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | (LRBG2) Message 3/24  NID\_BG=BG2  Packet 65   NID\_TSR   V\_TSR = V1  L\_TSR= L1  D\_TSR= D1 | | |  |
| 3 | The train starts the braking curve to the TSR. | DMI (O) | | Braking curve with V\_target = V1  Vtrain < Vpermitted | | |  |
| DMI (I) | |  | | |  |
| JRU | | V\_TRAIN < V\_PERMITTED  V\_TARGET = V1 | | |  |
| 4 | The EVC runs the distance at which the acknowledgement window of the transition to LSTM ASFA is shown to the driver. | DMI (O) | | Level STM ASFA acknowledgement is displayed | | |  |
| DMI (I) | |  | | |  |
| JRU | | START DISPLAYING TEXT MESSAGE (2)  Estimated front end=d-L-L\_DOUBTUNDER | | |  |
| 5 | The driver acknowledges the level transition. | DMI (O) | | Level STM ASFA acknowledgement disappears | | |  |
| DMI (I) | | Driver acknowledges the level transition. | | |  |
| JRU | | M\_DRIVERACTIONS = 10  STOP DISPLAYING TEXT MESSAGE (2) | | |  |
| 6 | The EVC runs the distance "d" or the balise group with level transition order to LSTM ASFA is read. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | (LRBG2)  Packet 41  D\_LEVELTR =32767  M\_LEVELTR = 1  NID\_STM = 0 (ASFA) | | |  |
| 7 | The EVC switches to LSTM ASFA. | DMI (O) | | Level STM symbol  SN mode symbol  Level STM ASFA transition announcement disappears | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL=1  M\_MODE=13  STOP DISPLAYING TEXT MESSAGE (1) | | |  |
| 8 | The train reports the level change to the RBC by a position report. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Message 136  Packet 0  M\_LEVEL=1 | | |  |
| Final state | | Level | | STM | | |  |
| Mode | | SN | | |  |
| Train Speed (km/h) | | NR | | |  |
| Other parameters | |  | | |  |
| Final Test Result | |  | | | | | |
| Field of Application | | Spain | | | | | |
| Briefing instructions | |  | | | | | |