|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *TEST CASE DESCRIPTION* | | | | | | | |
|  | | Code | Version | | Title | | |
| Test Case | | 1.4.3 | 3 | | Level transition from L1 to L0 + ASFA when the first signal after the transition border is closed. | | |
|
| Baseline applicable | | Baseline 2 (2.3.0.d) | | | | | |
| Test case author | | ADIF | | | | | |
| Test Objective(s) | | Verify that the transition from level 1 to level 0 + ASFA is performed correctly and that the transition fulfills the location and speed requirements. | | | | | |
| Diagram | |  | | | | | |
| Starting conditions | | Level | | | | 1 | |
| Mode | | | | FS | |
| Train Speed (km/h) | | | | Maximum permitted speed of the area | |
| Additional starting conditions | | | | The train is running in FS mode at the maximum permitted speed and approaching to the level transition border.  The first signal after the transition border is in stop aspect. | |
| Sequence of the Test Case | | Checkpoints | | | | | |
| Step | Step description | Interfaces | | Description of what to be tested at the interface | | | OK? |
| 1 | The train receives the level transition announcement via balise group. | DMI (O) | | Level 1  FS mode symbol  Level 0 transition announcement is displayed | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL = 2  M\_MODE = 0  Packet 41  D\_LEVELTR = D1  M\_LEVELTR = 0  L\_ACKLEVELTR = L1  START DISPLAYING TEXT MESSAGE (1) | | |  |
| 2 (\*) | The ETCS on-board unit changes the ASFA mode from EXT to AV/CONV. |  | |  | | |  |
| 3 | The EVC runs the distance “D1-L1” at which the acknowledgement window of the transition to Level 0 is shown to the driver. | DMI (O) | | Level 0 acknowledgement is displayed | | |  |
| DMI (I) | |  | | |  |
| JRU | | Estimated front end≥D1-L1-L\_DOUBTUNDER  START DISPLAYING TEXT MESSAGE (2) | | |  |
| 4 | The driver acknowledges the level transition. | DMI (O) | | Level 0 acknowledgement disappears | | |  |
| DMI (I) | | Driver acknowledges the level transition. | | |  |
| JRU | | M\_DRIVERACTIONS = 6  STOP DISPLAYING TEXT MESSAGE (2) | | |  |
| 5 | The EVC runs the distance "D1" or the balise group with level transition order to Level 0 is read. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Packet 41  D\_LEVELTR =32767  M\_LEVELTR = 0 | | |  |
| 6 | The EVC switches to Level 0. | DMI (O) | | Level 0 Symbol  UN mode symbol  L0 transition announcement disappears | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL=0  M\_MODE=4  STOP DISPLAYING TEXT MESSAGE (1) | | |  |
| 7 (\*) | The driver is able to see the marker boards and trackside signals ahead and the permitted speed at the transition point allows the train to respect the signaling speed restrictions in the ASFA area. |  | |  | | |  |
| 8 (\*) | The on board equipment runs in L0+ASFA and reads correctly the first ASFA balise after the level transition border. |  | |  | | |  |
| 9 (\*) | The train can stop at the first light signal in the ASFA area (at stop aspect) with comfort braking. |  | |  | | |  |
| Final state | | Level | | 0 | | |  |
| Mode | | UN | | |  |
| Train Speed (km/h) | | NR | | |  |
| Other parameters | |  | | |  |
| Final Test Result | |  | | | | | |
| Field of Application | | Spain | | | | | |
| Briefing instructions | | (\*) These steps verify functionality related to NF-27. | | | | | |