|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *TEST CASE DESCRIPTION* | | | | | | | |
|  | | Code | Version | | Title | | |
| Test Case | | 2.1.1 | 1 | | Level transition from LSTM LZB to L1. Standard operating conditions. | | |
|
| Baseline applicable | | Baseline 2 (2.3.0.d) | | | | | |
| Test case author | | ADIF | | | | | |
| Test Objective(s) | | Verify that the transition from level STM LZB to level 1 is performed correctly. | | | | | |
| Diagram | |  | | | | | |
| Starting conditions | | Level | | | | STM LZB | |
| Mode | | | | SN | |
| Train Speed (km/h) | | | | NR | |
| Additional starting conditions | | | | The train is running in LSTM LZB with transmission and approaching a BG with level 1 transition announcement and the signals ahead are in permissive aspect. | |
| Sequence of the Test Case | | Checkpoints | | | | | |
| Step | Step description | Interfaces | | Description of what to be tested at the interface | | | OK? |
| 1 | The train receives the level transition announcement via balise group. | DMI (O) | | Level 1 transition announcement | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL = 1  M\_MODE = 13  Packet 41  D\_LEVELTR = D1  M\_LEVELTR = 2  L\_ACKLEVELTR = L1 | | |  |
| 2 | The EVC runs the distance “D1-L1” at which the acknowledgement window of the transition to Level 1 is shown to the driver. | DMI (O) | | Level 1 Acknowledgement is displayed | | |  |
| DMI (I) | |  | | |  |
| JRU | | Estimated front end=D1-L1-L\_DOUBTUNDER | | |  |
| 3 | The driver acknowledges the level transition. | DMI (O) | | Level 1 Acknowledgement disappears | | |  |
| DMI (I) | | Driver acknowledges the level transition. | | |  |
| JRU | | M\_DRIVERACTIONS = 7 | | |  |
| 4 | The EVC receives a MA from a BG. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Packet 12  Packet 21  Packet 27 | | |  |
| 5 | The EVC runs the distance "D1" or the balise group with level transition order to L1 is read. | DMI (O) | |  | | |  |
| DMI (I) | |  | | |  |
| JRU | | Packet 41  D\_LEVELTR = 32767  M\_LEVELTR = 2 | | |  |
| 6 | Transition to L1 is performed. (with no abrupt changes in the permitted speed). | DMI (O) | | Level 1 Symbol  FS Symbol  Level 1 transition announcement disappears  Entering FS message | | |  |
| DMI (I) | |  | | |  |
| JRU | | M\_LEVEL= 2  M\_MODE = 0 | | |  |
| Final state | | Level | | 1 | | |  |
| Mode | | FS | | |  |
| Train Speed (km/h) | | NR | | |  |
| Other parameters | |  | | |  |
| Final Test Result | |  | | | | | |
| Field of Application | | Spain | | | | | |
| Briefing instructions | | Step 4 could take place at any moment between step 1 and step 5, both steps included.  In case the train is equipped with L0+LZB, the test case shall be adapted accordingly. | | | | | |